|  |  |  |
| --- | --- | --- |
| **BIRCOdicht NW 150 - 300 – In-line outfall unit with shut-off valve**  for 1- or 2-sided channel connection, including stainless steel L angle frame (V2A - also removable)  + Manually operated valve flap DN 150  + On request also with pneumatical valve flap  + PEHD lining  + Drain direction in accordance with the customer’s wishes  + PEHD-pipe socket DA 160 – SDR 17, 300 mm long  + Length 500 mm  + Width 470 mm  made of concrete C 40/50 according to EN 1433, up to load class F 900 as defined by EN 1433, with visible sealing joint  [ ] \_\_\_\_\_ pce in-line outfall unit(s) 1 piece, construction height   with angles 805 mm  delivery and installation according to manufacturer’s installation instructions.  Manufacturer: BIRCO GmbH Herrenpfädel 142, D 76532 Baden-Baden Phone +497221 - 5003-0; Fax +497221 - 5003-1149; www.birco.de | **Unit price** | **Total price** |
| **BIRCOdicht NW 150 - 300 – Gratings for in-line outfall unit with shut-off valve**  + Width 437 mm  + Height 45 mm  + With keybushing  load class according to DIN EN 1433, with 4 point per grating M12/A2-bolt fastening  [ ] \_\_\_\_\_ pce cast twofold slotted gratings black immersion-  lacquered, length 500 mm, load class F 900  delivery and installation according to manufacturer’s installation instructions.  Manufacturer:  BIRCO GmbH | **Unit price** | **Total price** |
| **BIRCOsolid NW 150 - 300 – Service key**  + For in-line outfall unit with shut-off valve  + For manuel operation  [ ] \_\_\_\_\_ pce service key  delivery.  Manufacturer: BIRCO GmbH | **Unit price** | **Total price** |