|  |  |  |
| --- | --- | --- |
| **BIRCOprotect NW 100 – Drainage channel with 1 % inbuilt fall with German Technical approval**+ Length 1000 mm+ Width at top 200 mm, width at bottom 205 mm+ Construction height at groove/tongue 180 to 280 mm+ With German Technical Approval (certificate no. Z-74.4-34)made of concrete C 40/50 according to EN 1433, up to load class F 900 as defined by EN 1433, with anchored 4 mm hot-dipped galvanized solid steel angles for combi-closure system (70 µm zinc coating), with visible sealing joint[ ] \_\_\_\_\_ m BIRCOprotect NW 100 channel no. 1 - 10including necessary end caps, delivery and installation according to manufacturer’s installation instructions.Manufacturer: BIRCO GmbHHerrenpfädel 142, D 76532 Baden-BadenPhone +497221 - 5003-0; Fax +497221 - 5003-1149; www.birco.de | **Unit price** | **Total price** |
| **BIRCOprotect NW 100 – Drainage channel without inbuilt fall with German Technical Approval**+ Length 500 mm (only for height 180 mm) / 1000 mm+ Width at top 200 mm, width at bottom 205 mm+ Construction height 180/230/280 mm+ With German Technical Approval (certificate no. Z-74.4-34)made of concrete C 40/50 according to EN 1433, up to load class F 900 as defined by EN 1433, with anchored 4 mm hot-dipped galvanized solid steel angles for combi-closure system (70 µm zinc coating), with visible safety sealing joint[ ] \_\_\_\_\_ m BIRCOprotect NW 100 channel no. 0/0, 5/0, 10/0 including necessary end caps, delivery and installation according to manufacturer’s installation instructions.Manufacturer: BIRCO GmbH | **Unit price** | **Total price** |
| **BIRCOprotect NW 100 – End caps and end caps with outlet DN 100**+ Width 200 mmMade of galvanized steel[ ] \_\_\_\_\_ pce of end cap for channel no. 0/0–3 / 4–7 / 8–10[ ] \_\_\_\_\_ pce of end cap with outlet DN 100 for channel no.  0/0 / 5/0 / 10/0[ ] \_\_\_\_\_ pce of end cap with outlet DA 110 x 6,3 – SDR17, PEHD for channel no. 0/0 / 5/0 / 10/0 length 300 mmdelivery.Manufacturer: BIRCO GmbH | **Unit price** | **Total price** |

|  |  |  |
| --- | --- | --- |
| **BIRCOprotect NW 100 – In-line outfall unit with PEHD pipe connector** for 1- or 2-sided channel connection**+** PP-silt bucket+ PEHD pipe connector DA 110x6,3 – SDR 17, length 300 mm + Length at top 500 mm, length at bottom 510 mm+ Width at top 200 mm, width at bottom 230mm,made of concrete C 40/50 according to EN 1433, up to load class F 900 as defined by EN 1433, with anchored 4 mm hot-dipped galvanized solid steel angles for combi-closure system (70 µm zinc coating), with visible safety sealing joint[ ] \_\_\_\_\_ pce of in-line outfall unit(s), 1 piece, construction  height 490 mmincluding necessary end caps, delivery and installation according to manufacturer’s installation instructions.Manufacturer: BIRCO GmbH | **Unit price** | **Total price** |
| **BIRCOprotect NW 100 – Gratings**+ Width 187 mm+ Height 30 mmload class according to DIN EN 1433, with 8-point per metre M12/A2-bolt fastening or Easylock fastening, mesh grating with4-point fastening per grating[ ] \_\_\_\_\_ pce cast slotted grating black immersion-lacquered, length 500 mm, load class C 250 / E 600 / F 900[ ] \_\_\_\_\_ pce cast slotted grating galvanized,  length 500 mm, load class E 600 [ ] \_\_\_\_\_ pce cast mesh grating black immersion-lacquered, length 500 mm, load class E 600[ ] \_\_\_\_\_ pce cast mesh grating galvanized, length 500 mm, load class E 600[ ] \_\_\_\_\_ pce mesh grating galvanized steel,  length 500 / 1000 mm, mesh width 30/30 mm, load class C 250 mesh width 30/12 mm, load class C 250 mesh width 20/30 mm, load class E 600 mesh width 20/12 mm, load class E 600delivery and installation according to manufacturer’s installation instructions.Manufacturer: BIRCO GmbH | **Unit price** | **Total price** |
| **BIRCOprotect NW 100 – Cutting of channels including grating** and painting or galvanizing of cut angles and gratings. For mesh gratings welding of end pieces and galvanizing. [ ] \_\_\_\_\_ 90° cut[ ] \_\_\_\_\_ Mitre cut according to degree specificationManufacturer: BIRCO GmbH | **Unit price** | **Total price** |

|  |  |  |
| --- | --- | --- |
| **BIRCOprotect NW 100 - Hole drilling of channel**[ ] \_\_\_\_\_ in horizontal / vertical direction, diameter DN 100[ ] \_\_\_\_\_ pce of silt bucket(s)Delivery.Manufacturer: BIRCO GmbH | **Unit price** | **Total price** |