|  |  |  |
| --- | --- | --- |
| **BIRCOprotect NW 150 – Drainage channel with 0.5 % inbuilt fall with German Technical approval**+ Length 1000 mm, + Width at top 250 mm, width at bottom 255 mm+ Construction height at groove/tongue 230 to 280 mm+ With German Technical Approval (certificate no. Z-74.4-34)made of concrete C 40/50 according to EN 1433, up to load class F 900 as defined by EN 1433, with anchored 4 mm hot-dipped galvanized solid steel angles for combi-closure system (70 µm zinc coating), with visible sealing joint[ ] \_\_\_\_\_ m BIRCOprotect NW 150 channel no. 1 - 10including necessary end caps, delivery and installation according to manufacturer’s installation instructions.Manufacturer: BIRCO GmbHHerrenpfädel 142, D 76532 Baden-BadenPhone +497221 - 5003-0; Fax +497221 - 5003-1149; www.birco.de | **Unit price** | **Total price** |
| **BIRCOprotect NW 150 – Drainage channel without inbuilt fall with German Technical Approval**+ Length 500 mm (only for height 230 mm)/1000 mm+ Width at top 250 mm, width at bottom 255 mm+ Construction height 230/255/280 mm+ With German Technical Approval (certificate no. Z-74.4-34)made of concrete C 40/50 according to EN 1433, up to load class F 900 as defined by EN 1433, with anchored 4 mm hot-dipped galvanized solid steel angles for combi-closure system (70 µm zinc coating), with visible safety sealing joint[ ] \_\_\_\_\_ m BIRCOprotect NW 150 channel no. 0/0, 5/0, 10/0including necessary end caps, delivery and installation according to manufacturer’s installation instructions.Manufacturer:BIRCO GmbH | **Unit price** | **Total price** |
| **BIRCOprotect NW 150 – End caps and end caps with outlet DN 150**+ Width 250 mmMade of galvanized steel[ ] \_\_\_\_\_ pce of end cap for channel no. 0/0–4 / 5– 7 / 8 – 10[ ] \_\_\_\_\_ pce of end cap with outlet DN 150 for channel no. 0/0  / 5/0 / 10/0[ ] \_\_\_\_\_ pce of end cap with outlet DA 160 x 9,1 – SDR17,  PEHD for channel no. 0/0 / 5/0 / 10/0, length 300 mm delivery.Manufacturer:BIRCO GmbH | **Unit price** | **Total price** |

|  |  |  |
| --- | --- | --- |
| **BIRCOprotect NW 150 – In-line outfall unit**  **with PEHD pipe connector** for 1- or 2-sided channel connection**+** PP-silt bucket + PEHD pipe connector DA 160x9,1 – SDR 17, length 300 mm+ Length at top 500 mm, length at bottom 510 mm+ Width at top 250 mm, width at bottom 260mm,made of concrete C 40/50 according to EN 1433, up to load class F 900 as defined by EN 1433, with anchored 4 mm hot-dipped galvanized solid steel angles for combi-closure system (70 µm zinc coating), with visible safety sealing joint[ ] \_\_\_\_\_ pce of in-line outfall unit(s), 1 piece, construction  height 710 mm, including necessary end caps, delivery and installation according to manufacturer’s installation instructions.Manufacturer:BIRCO GmbH | **Unit price** | **Total price** |
| **BIRCOprotect NW 150 – Gratings**+ Width 237 mm+ Height 30 mmload class according to DIN EN 1433, with 8-point per metre M12/A2-bolt fastening or Easylock fastening, mesh grating with4-point fastening per grating[ ] \_\_\_\_\_ pce cast slotted grating black immersion-lacquered, length 500 mm, load class C 250 / E 600 / F 900[ ] \_\_\_\_\_ pce cast slotted grating galvanized,  length 500 mm, load class E 600[ ] \_\_\_\_\_ pce cast mesh grating black immersion-lacquered, length 500 mm, load class E 600[ ] \_\_\_\_\_ pce cast mesh grating galvanized, length 500 mm, load class E 600[ ] \_\_\_\_\_ pce honeycomb gratings black immersion-lacquered, length 500 mm, load class E 600[ ] \_\_\_\_\_ pce honeycomb gratings galvanized, length 500 mm, load class E 600[ ] \_\_\_\_\_ pce mesh grating galvanized steel,  length 500 / 1000 mm, mesh width 30/30 mm, load class C 250 mesh width 30/15 mm, load class C 250 mesh width 20/30 mm, load class E 600 mesh width 20/12 mm, load class E 600delivery and installation according to manufacturer’s installation instructions.Manufacturer:BIRCO GmbH | **Unit price** | **Total price** |

|  |  |  |
| --- | --- | --- |
| **BIRCOprotect NW 150 – Cutting of channels including grating** and painting or galvanizing of cut angles and gratings. For mesh gratings welding of end pieces and galvanizing. [ ] \_\_\_\_\_ 90° cut[ ] \_\_\_\_\_ Mitre cut according to degree specificationManufacturer: BIRCO GmbH | **Unit price** | **Total price** |
| **BIRCOprotect NW 150 – Hole drilling of channel**[ ] \_\_\_\_\_ in horizontal / vertical direction, diameter DN 100[ ] \_\_\_\_\_ pce of silt bucket(s)Delivery.Manufacturer:BIRCO GmbH | **Unit price** | **Total price** |