|  |  |  |
| --- | --- | --- |
| **BIRCOprotect NW 200 – Drainage channel with 0.5 % inbuilt fall with German Technical approval**+ Length 1000 mm+ Width at top 330 mm, width at bottom 335 mm+ Construction height at groove/tongue 310 to 360 mm+ With German Technical Approval (certificate no. Z-74.4-34)made of concrete C 40/50 according to EN 1433, up to load class F 900 as defined by EN 1433, with anchored 4 mm hot-dipped galvanized solid steel angles for combi-closure system (70 µm zinc coating), with visible sealing joint[ ] \_\_\_\_\_ m BIRCOprotect NW 200 channel no. 1 - 10including necessary end caps, delivery and installation according to manufacturer’s installation instructions.Manufacturer: BIRCO GmbHHerrenpfädel 142, D 76532 Baden-BadenPhone +497221 - 5003-0; Fax +497221 - 5003-1149; www.birco.de | **Unit price** | **Total price** |
| **BIRCOprotect NW 200 – Drainage channel without inbuilt fall with German Technical Approval**+ Length 500 mm (only for height 310 mm)/1000 mm+ Width at top 330 mm, width at bottom 335 mm+ Construction height 310/335/360 mm+ With German Technical Approval (certificate no. Z-74.4-34)made of concrete C 40/50 according to EN 1433, up to load class F 900 as defined by EN 1433, with anchored 4 mm hot-dipped galvanized solid steel angles for combi-closure system (70 µm zinc coating), with visible safety sealing joint[ ] \_\_\_\_\_ m BIRCOprotect NW 200 channelincluding necessary end caps, delivery and installation according to manufacturer’s installation instructions.Manufacturer:BIRCO GmbH | **Unit price** | **Total price** |
| **BIRCOprotect NW 200 – End caps and end caps with outlet DN 200**+ Width 330 mmMade of galvanized steel[ ] \_\_\_\_\_ pce of end cap for channel no. 0/0–6 / 7–10[ ] \_\_\_\_\_ pce of end cap with outlet DN 200 for channel no. 0/0  / 5/0 / 10/0[ ] \_\_\_\_\_ pce of end cap with outlet DA 200 x 4,9 – SDR 41,  PEHD for channel no. 0/0 / 5/0 / 10/0, length 300 mm delivery.Manufacturer:BIRCO GmbH | **Unit price** | **Total price** |

|  |  |  |
| --- | --- | --- |
| **BIRCOprotect NW 200 – In-line outfall unit**  **with PEHD pipe connector** for 1- or 2-sided channel connection+ Galvanized silt bucket+ PEHD pipe connector DA 200 x 4,9 – SDR 41, length 300 mm+ Length at top 500 mm, length at bottom 510 mm+ Width at top 330 mm, width at bottom 345mmmade of concrete C 40/50 according to EN 1433, up to load class F 900 as defined by EN 1433, with anchored 4 mm hot-dipped galvanized solid steel angles for combi-closure system (70 µm zinc coating), with visible safety sealing joint[ ] \_\_\_\_\_ pce of in-line outfall unit(s), 1 piece, construction  height 725 mm,including necessary end caps, delivery and installation according to manufacturer’s installation instructions.Manufacturer:BIRCO GmbH | **Unit price** | **Total price** |
| **BIRCOprotect NW 200 – Gratings**+ Width 317 mm+ Width 35 mmload class according to DIN EN 1433, with 8-point per metre M12/A2-bolt fastening [ ] \_\_\_\_\_ pce cast slotted grating black immersion-lacquered, length 500 mm, load class F 900delivery and installation according to manufacturer’s installation instructions.Manufacturer:BIRCO GmbH | **Unit price** | **Total price** |
| **BIRCOprotect NW 200 – Cutting of channels including grating** and painting or galvanizing of cut angles and gratings.[ ] \_\_\_\_\_ 90° cut[ ] \_\_\_\_\_ Mitre cut according to degree specificationManufacturer:BIRCO GmbH | **Unit price** | **Total price** |
| **BIRCOprotect NW 200 – Hole drilling of channel**[ ] \_\_\_\_\_ in horizontal / vertical direction, diameter DN 200[ ] \_\_\_\_\_ pce of silt bucket(s)Delivery.Manufacturer:BIRCO GmbH | **Unit price** | **Total price** |