|  |  |  |
| --- | --- | --- |
| **BIRCOsolid NW 200 – Grid channel type I without inbuilt fall, with German Technical Approval, ASR-resistant**+ With anchor sleeves for smooth laying+ With interior lifting anchor for precise installation+ Length 1000 mm / 1500 mm / 4000 mm+ Width 550 mm+ Construction height 415 mm+ German Technical Approval certificate no. Z-74.4-33made of concrete C 40/50 according to EN 1433, up to load class F 900 as defined by EN 1433, with anchored 4 mm hot-dipped galvanized solid steel angles for combi-closure system (70 µm zinc coating), with visible sealing joint[ ] \_\_\_\_\_ m BIRCOsolid NW 200 channelincluding necessary end caps, delivery and installation according to manufacturer’s installation instructions.Manufacturer: BIRCO GmbHHerrenpfädel 142, D 76532 Baden-BadenPhone +497221 - 5003-0; Fax +497221 - 5003-1149; www.birco.de | **Unit price** | **Total price** |
| **BIRCOsolid NW 200 – End caps and end caps with outlet DN 200**+ Width 550 mmmade of galvanized steel[ ] \_\_\_\_\_ pce of end cap(s) for channel no. 0/0 [ ] \_\_\_\_\_ pce of end cap(s) with outlet DN 200 for channel  no. 0/0[ ] \_\_\_\_\_ pce of end cap(s) with outlet DA 225 PEHD for channel no. 0/0, factory assembleddelivery.Manufacturer: BIRCO GmbH | **Unit price** | **Total price** |

|  |  |  |
| --- | --- | --- |
| **BIRCOsolid NW 200 – In-line outfall unit with cast-in pipe connector** for 1- or 2-sided channel connection+ Length 500 mm+ Width at top 550mm, width at bottom 585 mm+ Galvanized silt bucket+ Cast-in pipe connector for DN 200 pipe**+** Without odour trapmade of concrete C 40/50 according to EN 1433, up to load class F 900 as defined by EN 1433, with anchored 4 mm hot-dipped galvanized solid steel angles for combi-closure system (70 µm zinc coating), with visible sealing joint[ ] \_\_\_\_\_ pce of in-line outfall unit, 1 piece, construction  height 980 mmincluding necessary end caps, delivery and installation according to manufacturer’s installation instructions.Manufacturer: BIRCO GmbH | **Unit price** | **Total price** |
| **BIRCOsolid NW 200 – In-line outfall unit with PEHD pipe connector** for 1- or 2-sided channel connection+ Length 500 mm+ Width 550mm+ Galvanized silt bucket+ PEHD pipe connector DA 225x12,8 – SDR 17, length 300 mmmade of concrete C 40/50 according to EN 1433, up to load class F 900 as defined by EN 1433, with anchored 4 mm hot-dipped galvanized solid steel angles for combi-closure system (70 µm zinc coating), with visible sealing joint[ ] \_\_\_\_\_ pce in-line outfall unit, 1 pipe, construction height, 980 mmincluding necessary end caps, delivery and installation according to manufacturer’s installation instructions.Manufacturer: BIRCO GmbH | **Unit price** | **Total price** |

|  |  |  |
| --- | --- | --- |
| **BIRCOsolid NW 200 – Gratings**+ Width 317 mm+ Height Höhe 35 mmload class according to DIN EN 1433, with 4-point per grating M12/A2-bolt fastening[ ] \_\_\_\_\_ pce cast slotted grating black immersion-lacquered, length 500 mm, load class F 900including necessary end caps, delivery and installation according to manufacturer’s installation instructions.Manufacturer:BIRCO GmbH | **Unit price** | **Total price** |
| **BIRCOsolid NW 200 – Shut-off outfall unit NW 400 for channel NW 200** for 1- or 2-sided channel connection up to NW 400 (on request with end caps / adapter caps for channel connection mounted ex-works)+ Manually operated valve flap DN 200+ On request also with electrical or pneumatical valve flap+ Galvanized silt bucket+ PEHD pipe connector DA 225 x 12,8 – SDR 17, length 300 mm+ Pipe connector at right angles to channel line+ Not covered by German Technical Approval certificate+ Length 500 mm+ Width at top 550 mm, width at bottom 610 mm,made of concrete C 40/50 according to EN 1433, up to load class F 900 as defined by EN 1433, with anchored 4 mm hot-dipped galvanized solid steel angles for combi-closure system (70 µm zinc coating), with visible safety sealing joint[ ] \_\_\_\_\_ pce shut-off outfall unit, 1-piece, construction height  980 mmincluding necessary end caps, delivery and installation according to manufacturer’s installation instructions.Manufacturer:BIRCO GmbH | **Unit price** | **Total price** |

|  |  |  |
| --- | --- | --- |
| **BIRCOsolid NW 200 – Gratings for shut-off outfall unit NW 300**+ With key bushing+ Width 537 mm+ Height 45 mmload class according to DIN EN 1433, with 4-point per grating M16/A2-bolt fastening[ ] \_\_\_\_\_ pce cast twofold slotted grating black immersion- lacquered, length 500 mm, load class E 600delivery and installation according to manufacturer’s installation instructions Manufacturer:BIRCO GmbH | **Unit price** | **Total price** |
| **BIRCOsolid NW 200 – Cutting of channel including grating** and painting or galvanizing of cut angles and gratings.[ ] \_\_\_\_\_ 90° cut[ ] \_\_\_\_\_ Mitre cut according to degree specificationManufacturer:BIRCO GmbH | **Unit price** | **Total price** |
| **BIRCOsolid NW 200 – Hole drilling of channel**[ ] \_\_\_\_\_ in horizontal / vertical direction, diameter DN 200[ ] \_\_\_\_\_ pce of silt bucket(s)Delivery.Manufacturer:BIRCO GmbH | **Unit price** | **Total price** |
| **BIRCOsolid NW 200 – Hangers for RD 16 piping**[ ] \_\_\_\_\_ Hanger RD 16DeliveryManufacturer:BIRCO GmbH | **Unit price** | **Total price** |
| **BIRCOsolid NW 200 – Service key**+ For shut-off outfall unit+ For manual operation[ ] \_\_\_\_\_ pce service keyManufacturer:BIRCO GmbH | **Unit price** | **Total price** |