|  |  |  |
| --- | --- | --- |
| **BIRCOsolid slot channel type I without inbuilt fall with German Technical Approval, ASR resistant**  + Monolithic concrete body  + Interrupted slot, slot width 30/50 mm  + Length 4000 mm  + Width at top 540 mm, width at bottom 500 mm  + Construction height 550 mm  + cast honeycomb grating black immersion-lacquered, length   500 mm, load class (500/287/30, mesh width 20/75 mm)  + German Technical Approval certificate No. Z-74.4-62  made of concrete C 40/50 according to EN 1433, up to load class F 900 as defined by EN 1433, with anchored 4 mm hot-dipped galvanized solid steel angles for combi-closure system (70 µm zinc coating), with visible safety sealing joint  [ ] \_\_\_\_\_ m BIRCOsolid slot channel  including necessary end caps, delivery and installation according to manufacturer’s installation instructions.  Manufacturer:  BIRCO GmbH Herrenpfädel 142, D 76532 Baden-Baden Phone +497221 - 5003-0; Fax +497221 - 5003-1149; www.birco.de | **Unit price** | **Total price** |
| **BIRCOsolid slot channel – end cap**  + Width 500 mm  Made of galvanized steel  [ ] \_\_\_\_\_ pce of end cap, construction height 500 mm  delivery.  Manufacturer:  BIRCO GmbH | **Unit price** | **Total price** |
| **BIRCOsolid slot channel – In-line outfall unit with cast-in pipe connector** for 1- or 2-sided channel connection  + Galvanized silt bucket  + Cast-in pipe connector for DN 200 pipe  **+** Without odour trap  + Length 500 mm  + Width at top 540 mm, width at bottom 580 mm  made of concrete C 40/50 according to EN 1433, up to load class F 900 as defined by EN 1433, with anchored 4 mm hot-dipped galvanized solid steel angles for combi-closure system (70 µm zinc coating), with visible sealing joint  [ ] pce of in-line outfall unit, 1-piece,   construction height 980 mm  including necessary end caps, delivery and installation according to manufacturer’s installation instructions.  Manufacturer:  BIRCO GmbH | **Unit price** | **Total price** |

|  |  |  |
| --- | --- | --- |
| **BIRCOsolid slot channel – – In-line outfall unit with PEHD pipe connector** for 1- or 2-sided channel connection  + Galvanized silt bucket  + PEHD pipe support DA 225 x 12,8 – SDR 17, length 300 mm  + Length 500 mm  + Width 540 mm  made of concrete C 40/50 according to EN 1433, up to load class F 900 as defined by EN 1433, with anchored 4 mm hot-dipped galvanized solid steel angles for combi-closure system (70 µm zinc coating), with visible sealing joint  [ ] \_\_\_\_\_ pce in-line outfall unit, 1 piece, construction height  980 mm  including necessary end caps, delivery and installation according to manufacturer’s installation instructions.  Manufacturer:  BIRCO GmbH | **Unit price** | **Total price** |
| **BIRCOsolid slot channel – gratings for in-line outfall units**  + Width 287 mm  + Height 35 mm  load class according to DIN EN 1433, with 4-point per grating M12/A2-bolt fastening  [ ] \_\_\_\_\_ pce cast honeycomb grating black immersion-  lacquered, length 500 mm, load class F 900  delivery and installation according to manufacturer’s installation instructions  Manufacturer:  BIRCO GmbH | **Unit price** | **Total price** |
| **BIRCOsolid slot channel – laying spades**  + DEHA lifting system  + 2 lifting spades  [ ] rent  [ ] purchase  Delivery.  Manufacturer:  BIRCO GmbH | **Unit price** | **Total price** |