|  |  |  |
| --- | --- | --- |
| **BIRCOsolid slot channel type I without inbuilt fall with German Technical Approval, ASR resistant**+ Monolithic concrete body+ Interrupted slot, slot width 30/50 mm+ Length 4000 mm+ Width at top 540 mm, width at bottom 500 mm+ Construction height 550 mm+ cast honeycomb grating black immersion-lacquered, length  500 mm, load class (500/287/30, mesh width 20/75 mm)+ German Technical Approval certificate No. Z-74.4-62made of concrete C 40/50 according to EN 1433, up to load class F 900 as defined by EN 1433, with anchored 4 mm hot-dipped galvanized solid steel angles for combi-closure system (70 µm zinc coating), with visible safety sealing joint[ ] \_\_\_\_\_ m BIRCOsolid slot channelincluding necessary end caps, delivery and installation according to manufacturer’s installation instructions.Manufacturer: BIRCO GmbHHerrenpfädel 142, D 76532 Baden-BadenPhone +497221 - 5003-0; Fax +497221 - 5003-1149; www.birco.de | **Unit price** | **Total price** |
| **BIRCOsolid slot channel – end cap**+ Width 500 mmMade of galvanized steel[ ] \_\_\_\_\_ pce of end cap, construction height 500 mmdelivery.Manufacturer: BIRCO GmbH | **Unit price** | **Total price** |
| **BIRCOsolid slot channel – In-line outfall unit with cast-in pipe connector** for 1- or 2-sided channel connection+ Galvanized silt bucket+ Cast-in pipe connector for DN 200 pipe**+** Without odour trap+ Length 500 mm+ Width at top 540 mm, width at bottom 580 mmmade of concrete C 40/50 according to EN 1433, up to load class F 900 as defined by EN 1433, with anchored 4 mm hot-dipped galvanized solid steel angles for combi-closure system (70 µm zinc coating), with visible sealing joint[ ] pce of in-line outfall unit, 1-piece,  construction height 980 mmincluding necessary end caps, delivery and installation according to manufacturer’s installation instructions.Manufacturer: BIRCO GmbH | **Unit price** | **Total price** |

|  |  |  |
| --- | --- | --- |
| **BIRCOsolid slot channel – – In-line outfall unit with PEHD pipe connector** for 1- or 2-sided channel connection+ Galvanized silt bucket+ PEHD pipe support DA 225 x 12,8 – SDR 17, length 300 mm+ Length 500 mm+ Width 540 mmmade of concrete C 40/50 according to EN 1433, up to load class F 900 as defined by EN 1433, with anchored 4 mm hot-dipped galvanized solid steel angles for combi-closure system (70 µm zinc coating), with visible sealing joint[ ] \_\_\_\_\_ pce in-line outfall unit, 1 piece, construction height 980 mmincluding necessary end caps, delivery and installation according to manufacturer’s installation instructions.Manufacturer: BIRCO GmbH | **Unit price** | **Total price** |
| **BIRCOsolid slot channel – gratings for in-line outfall units**+ Width 287 mm+ Height 35 mmload class according to DIN EN 1433, with 4-point per grating M12/A2-bolt fastening[ ] \_\_\_\_\_ pce cast honeycomb grating black immersion- lacquered, length 500 mm, load class F 900delivery and installation according to manufacturer’s installation instructions Manufacturer: BIRCO GmbH | **Unit price** | **Total price** |
| **BIRCOsolid slot channel – laying spades**+ DEHA lifting system + 2 lifting spades[ ] rent[ ] purchaseDelivery.Manufacturer: BIRCO GmbH | **Unit price** | **Total price** |