|  |  |  |
| --- | --- | --- |
| **BIRCOcanal NW 400 – Supply channels with angles**+ Length 1000 mm / 2000 mm+ External width 550 mm, internal width 400 mm+ External construction height 480 mm, internal height 360 mmmade of concrete C 40/50, CE compliance with EN 1433, up to load class F 900 as defined by EN 1433, with anchored 4 mm hot-dipped galvanized solid steel angles for combi-closure system (70 µm zinc coating), with safety sealing joint[ ] \_\_\_\_\_ m BIRCOcanal NW 400 channel length 1000/2000 mm  with cast-in mounting rails[ ] \_\_\_\_\_ m BIRCOcanal NW 400 channel length 1000/2000 mm  without mounting rails[ ] Sealing with SF-Connectincluding the necessary end caps, delivery and installation according to manufacturer’s installation instructions.Manufacturer: BIRCO GmbHHerrenpfädel 142, D 76532 Baden-BadenPhone +497221 - 5003-0; Fax +497221 - 5003-1219; www.birco.de | **Unit price** | **Total price** |
| **BIRCOcanal NW 400 – Gratings for supply channels with angles**+ Width 537 mm+ Height 45 mmload class according to DIN EN 1433, with 8 point per metre M16/A2-bolt fastening or Easylock fastening[ ] \_\_\_\_\_ pce bulb ductile iron cover(s) black immersion- lacquered, length 500 mm, load class E 600[ ] \_\_\_\_\_ pce bulb ductile iron cover(s) galvanized,  length 500 mm, load class E 600delivery and installation according to manufacturer’s installation instructions.Manufacturer:BIRCO GmbH | **Unit price** | **Total price** |
| **BIRCOcanal NW 400 – Cutting of channels including grating** and painting or galvanizing of cut angles and gratings.[ ] \_\_\_\_\_ Channel section 90°[ ] \_\_\_\_\_ Mitre cut according to degree specificationManufacturer:BIRCO GmbH | **Unit price** | **Total price** |
| **BIRCOcanal NW 400 – Drilled hole in channel base**[ ] \_\_\_\_\_ in horizontal / vertical direction, diameter DN 300Delivery.Manufacturer:BIRCO GmbH | **Unit price** | **Total price** |