|  |  |  |
| --- | --- | --- |
| **BIRCOcanal – Lifting loops**+ For mechanical installation of concrete covers+ For mechanical installation of supply channels without angles[ ] \_\_\_\_\_ pce lifting loops RD12 for NW 200 - 500[ ] \_\_\_\_\_ pce lifting loops RD14 for NW 700 - 1000Delivery.Manufacturer: BIRCO GmbHHerrenpfädel 142, D 76532 Baden-BadenPhone +497221 - 5003-0; Fax +497221 - 5003-1219; www.birco.de | **Unit price** | **Total price** |
| **BIRCOcanal – Side strips** + As support for BIRCOcanal concrete covers without angles+ Hot-dipped galvanized+ 1 or 2-sided+ Length 1000 mm+ Height 220 mm[ ] \_\_\_\_\_ pce side strips 1-sided, NW 200 – 700 / NW 1000  material thickness 5 mm[ ] \_\_\_\_\_ pce side strips 2-sided, NW 200 – 700 / NW 1000  material thickness 5 mmDelivery.Manufacturer:BIRCO GmbH | **Unit price** | **Total price** |
| **BIRCOcanal – Sealing tape**+ Flexible liner+ Between BIRCOcanal supply channel without angles and  reinforced grade concrete cover+ Self adhesive [ ] \_\_\_\_\_ m sealing tape, 50/6 mmDelivery.ManufacturerBIRCO GmbH | **Unit price** | **Total price** |