|  |  |  |
| --- | --- | --- |
| **BIRCOmassiv NW 200 – Drainage channel type I without inbuilt fall**+ Width at angle 500 mm, width at bottom 505 mm+ Construction height 415 mm+ With 8-point per metre anti-sliding safety studs of the gratingmade of constructively reinforced concrete C 40/50, CE compliance with EN 1433, up to load class F 900 as defined by EN 1433, with anchored one-piece hot-dipped galvanized surface protection, with safety sealing joint[ ] \_\_\_\_\_ m BIRCOmassiv NW 200 channel No. 0/0, with  galvanized surface protection,  length 1000 / 2000 mm[ ] Sealing with SF-Connectincluding the necessary end caps, delivery and installation according to manufacturer’s installation instructions.Manufacturer: BIRCO GmbHHerrenpfädel 142, D 76532 Baden-BadenPhone +497221 - 5003-0; Fax +497221 - 5003-1219; www.birco.de | **Unit price** | **Total price** |
| **BIRCOmassiv NW 200 – End caps and end caps with outlet DN 150**+ Width 500 mm+ for construction height 415 mmmade of galvanized steel[ ] \_\_\_\_\_ pce. of end cap(s)[ ] \_\_\_\_\_ pce. of end cap(s) with outlet DN 200delivery.Manufacturer: BIRCO GmbH | **Unit price** | **Total price** |
| **BIRCOmassiv NW 200 – Ring nut M12**+ For installation of concrete channelsmade of galvanized steel[ ] \_\_\_\_\_ pce of ring nut(s)delivery.Manufacturer:BIRCO GmbH | **Unit price** | **Total price** |

|  |  |  |
| --- | --- | --- |
| **BIRCOmassiv NW 200 – In-line outfall unit** for 1- or 2-sided channel connection+ Length 500 mm+ Width at angle 500 mm, width at bottom 500mm+ With 4-point anti-sliding safety studs of the gratingmade of constructively reinforced concrete C 40/50, CE compliance with EN 1433, up to load class F 900 as defined by EN 1433, with anchored one-piece hot-dipped galvanized surface protection, with safety sealing joint[ ] \_\_\_\_\_ pce of in-line outfall unit(s), 1 piece, construction  height 980 mm, with galvanized surface protection, integrated socket for DN 200 pipe connection, without  odour trap[ ] Sealing with SF-Connectincluding the necessary end caps, delivery and installation according to manufacturer’s installation instructions.Manufacturer: BIRCO GmbH | **Unit price** | **Total price** |
| **BIRCOmassiv NW 200 – Gratings**+ Width 287 mm+ Height 30 mmload class according to DIN EN 1433, 8 point per metre M12/A2 self-locking nuts[ ] \_\_\_\_\_ pce ductile iron slotted gratings black immersion- lacquered, length 500 mm, load class E 600 / F 900[ ] \_\_\_\_\_ pce ductile iron honeycomb gratings black immersion- lacquered, length 500 mm, load class E 600 / F 900delivery and installation according to manufacturer’s installation instructions Manufacturer:BIRCO GmbH | **Unit price** | **Total price** |
| **BIRCOmassiv NW 200 – Cutting of channels including grating** and painting or galvanizing of cut angles and gratings. [ ] \_\_\_\_\_ Channel section 90°[ ] \_\_\_\_\_ Mitre cut according to degree specificationManufacturer: BIRCO GmbH | **Unit price** | **Total price** |
| **BIRCOmassiv NW 200 – Hole drilling of channel**[ ] \_\_\_\_\_ in horizontal / vertical direction, diameter DN 200[ ] \_\_\_\_\_ pce of silt bucket(s)Delivery.Manufacturer: BIRCO GmbH | **Unit price** | **Total price** |