|  |  |  |
| --- | --- | --- |
| **BIRCOplus NW 100 – Drainage channel with 0.5 % inbuilt fall**  + Length 1000 mm  + Width at top 160 mm, width at bottom 163 mm  + Construction height at groove/tongue 165 to 215 mm  made of concrete C 40/50 according to EN 1433, up to load class C 250 as defined by EN 1433, with safety sealing joint  [ ] \_\_\_\_\_ m BIRCOplus NW 100 channel No. 1 - 10  [ ] Sealing with SF-Connect  including necessary end caps, delivery and installation according to manufacturer’s installation instructions.  Manufacturer:  BIRCO GmbH Herrenpfädel 142, D 76532 Baden-Baden Phone +497221 - 5003-0; Fax +497221 - 5003-1219; www.birco.de | **Unit price** | **Total price** |
| **BIRCOplus NW 100 – Drainage channel without inbuilt fall**  + Length 500 mm (just height 165 mm)/1000 mm  + Width at top 160 mm, width at bottom 163 mm  + Construction height 165/190/215 mm  made of concrete C 40/50 according to EN 1433, up to load class C 250 as defined by EN 1433, with safety sealing joint  [ ] \_\_\_\_\_ m BIRCOplus NW 100 channel No. 0/0, 5/0, 10/0  [ ] Sealing with SF-Connect  including necessary end caps, delivery and installation according to manufacturer’s installation instructions.  Manufacturer:  BIRCO GmbH | **Unit price** | **Total price** |
| **BIRCOplus NW 100 – End caps and end caps with outlet DN 100**  + width 160 mm  made of galvanized steel  [ ] \_\_\_\_\_ pce. of end cap for channel no. 0/0 – 2 / 3 – 6 / 7 - 10  [ ] \_\_\_\_\_ pce. of end cap with outlet DN 100 for channel no. 0/0 / 5/0 / 10/0  delivery.  Manufacturer:  BIRCO GmbH | **Unit price** | **Total price** |

|  |  |  |
| --- | --- | --- |
| **BIRCOplus NW 100 – – In-line outfall unit** for 1- or 2-sided channel connection  + PP odour trap  + Length at top 500 mm, length at bottom 510 mm  + Width at top 160 mm, width at bottom 185 mm  made of concrete C 40/50 according to EN 1433, up to load class C 250 as defined by EN 1433, galvanized silt bucket, with safety sealing joint  [ ] \_\_\_\_\_ pce in-line outfall unit, one-piece, construction height 490 mm, integrated socket for DN 100 pipe connection  [ ] Sealing with SF-Connect  including necessary end caps, delivery and installation according to manufacturer’s installation instructions.  Manufacturer:  BIRCO GmbH | **Unit price** | **Total price** |
| **BIRCOplus NW 100 – Gratings**  + Width 158 mm  load class C 250 as defined by EN 1433  [ ] \_\_\_\_\_ pce. ductile iron slotted gratings black immersion-  lacquered, including 2-point per metre M12/A bolt   connection with locking bracket, length 500 mm, load   class C 250  [ ] \_\_\_\_\_ pce. clamped slotted steel grating made of hot-dipped   galvanized steel, length 500 / 1000 mm, load class   A 15  [ ] \_\_\_\_\_ pce clamped mesh grating made of hot-dipped   galvanized steel, mesh width 30-16 / 30-10 mm  length 500 / 1000 mm, load class B 125  delivery and installation according to manufacturer’s installation instructions  Manufacturer:  BIRCO GmbH | **Unit price** | **Total price** |
| **BIRCOplus NW 100 – Outfall unit 30/30**  + PP odour trap  + Length 300 mm  + Width at top 300 mm, width at bottom 320 mm  made of concrete C 40/50 according to EN 1433, up to load class B 125 as defined by EN 1433, PP silt bucket  [ ] \_\_\_\_\_ pce outfall unit, one-piece, construction height   420 mm, integrated socket for DN 100 pipe connection  delivery and installation according to manufacturer’s installation instructions  Manufacturer:  BIRCO GmbH | **Unit price** | **Total price** |

|  |  |  |
| --- | --- | --- |
| **BIRCOplus NW 100 – Gratings for outfall unit 30/30**  + Width 300 mm  load class C 250 as defined by EN 1433  [ ] \_\_\_\_\_ pce. clamped slotted steel grating made of hot-dipped   galvanized steel, length 300 mm, load class A 15  [ ] \_\_\_\_\_ pce. clamped mesh grating made of hot-dipped   galvanized steel, length 300 mm, mesh width 30/16   mm, load class B 125  delivery and installation according to manufacturer’s installation instructions  Manufacturer:  BIRCO GmbH | **Unit price** | **Total price** |
| **BIRCOplus NW 100 – Outfall unit 19/19**  + PP odour trap  + Length 230 mm  + Width 230 mm  made of concrete C 40/50, up to load class A 15 according to EN 1433, PP silt bucket  [ ] \_\_\_\_\_ pce. outfall unit, one-piece, construction height 205 mm, integrated socket for DN 100 pipe connection, with ductile iron grating  [ ] \_\_\_\_\_ pce. outfall unit, one-piece, construction height 205 mm, integrated socket for DN 100 pipe connection, with mesh grating  delivery and installation according to manufacturer’s installation instructions  Manufacturer:  BIRCO GmbH | **Unit price** | **Total price** |
| **BIRCOplus NW 100 – Cutting of channels including grating** and painting or galvanizing of cut angles and gratings. For mesh gratings welding of end pieces and galvanizing.  [ ] \_\_\_\_\_ 90° cut  [ ] \_\_\_\_\_ Mitre cut according to degree specification  Manufacturer:  BIRCO GmbH | **Unit price** | **Total price** |
| **BIRCOplus NW 100 – Hole drilling of channel**  [ ] \_\_\_\_\_ in horizontal / vertical direction, diameter DN 100  [ ] \_\_\_\_\_ pce of silt bucket(s)  delivery.  Manufacturer:  BIRCO GmbH | **Unit price** | **Total price** |