|  |  |  |
| --- | --- | --- |
| **BIRCOplus NW 100 – Drainage channel with 0.5 % inbuilt fall**+ Length 1000 mm+ Width at top 160 mm, width at bottom 163 mm+ Construction height at groove/tongue 165 to 215 mmmade of concrete C 40/50 according to EN 1433, up to load class C 250 as defined by EN 1433, with safety sealing joint[ ] \_\_\_\_\_ m BIRCOplus NW 100 channel No. 1 - 10[ ] Sealing with SF-Connectincluding necessary end caps, delivery and installation according to manufacturer’s installation instructions.Manufacturer: BIRCO GmbHHerrenpfädel 142, D 76532 Baden-BadenPhone +497221 - 5003-0; Fax +497221 - 5003-1219; www.birco.de | **Unit price** | **Total price** |
| **BIRCOplus NW 100 – Drainage channel without inbuilt fall**+ Length 500 mm (just height 165 mm)/1000 mm+ Width at top 160 mm, width at bottom 163 mm+ Construction height 165/190/215 mmmade of concrete C 40/50 according to EN 1433, up to load class C 250 as defined by EN 1433, with safety sealing joint [ ] \_\_\_\_\_ m BIRCOplus NW 100 channel No. 0/0, 5/0, 10/0[ ] Sealing with SF-Connectincluding necessary end caps, delivery and installation according to manufacturer’s installation instructions.Manufacturer: BIRCO GmbH | **Unit price** | **Total price** |
| **BIRCOplus NW 100 – End caps and end caps with outlet DN 100**+ width 160 mmmade of galvanized steel [ ] \_\_\_\_\_ pce. of end cap for channel no. 0/0 – 2 / 3 – 6 / 7 - 10[ ] \_\_\_\_\_ pce. of end cap with outlet DN 100 for channel no. 0/0 / 5/0 / 10/0delivery.Manufacturer: BIRCO GmbH | **Unit price** | **Total price** |

|  |  |  |
| --- | --- | --- |
| **BIRCOplus NW 100 – – In-line outfall unit** for 1- or 2-sided channel connection+ PP odour trap+ Length at top 500 mm, length at bottom 510 mm+ Width at top 160 mm, width at bottom 185 mmmade of concrete C 40/50 according to EN 1433, up to load class C 250 as defined by EN 1433, galvanized silt bucket, with safety sealing joint[ ] \_\_\_\_\_ pce in-line outfall unit, one-piece, construction height 490 mm, integrated socket for DN 100 pipe connection[ ] Sealing with SF-Connectincluding necessary end caps, delivery and installation according to manufacturer’s installation instructions.Manufacturer: BIRCO GmbH | **Unit price** | **Total price** |
| **BIRCOplus NW 100 – Gratings**+ Width 158 mmload class C 250 as defined by EN 1433[ ] \_\_\_\_\_ pce. ductile iron slotted gratings black immersion- lacquered, including 2-point per metre M12/A bolt  connection with locking bracket, length 500 mm, load  class C 250[ ] \_\_\_\_\_ pce. clamped slotted steel grating made of hot-dipped  galvanized steel, length 500 / 1000 mm, load class  A 15[ ] \_\_\_\_\_ pce clamped mesh grating made of hot-dipped  galvanized steel, mesh width 30-16 / 30-10 mm length 500 / 1000 mm, load class B 125delivery and installation according to manufacturer’s installation instructionsManufacturer: BIRCO GmbH | **Unit price** | **Total price** |
| **BIRCOplus NW 100 – Outfall unit 30/30** + PP odour trap+ Length 300 mm+ Width at top 300 mm, width at bottom 320 mmmade of concrete C 40/50 according to EN 1433, up to load class B 125 as defined by EN 1433, PP silt bucket[ ] \_\_\_\_\_ pce outfall unit, one-piece, construction height  420 mm, integrated socket for DN 100 pipe connectiondelivery and installation according to manufacturer’s installation instructionsManufacturer: BIRCO GmbH | **Unit price** | **Total price** |

|  |  |  |
| --- | --- | --- |
| **BIRCOplus NW 100 – Gratings for outfall unit 30/30**+ Width 300 mmload class C 250 as defined by EN 1433[ ] \_\_\_\_\_ pce. clamped slotted steel grating made of hot-dipped  galvanized steel, length 300 mm, load class A 15[ ] \_\_\_\_\_ pce. clamped mesh grating made of hot-dipped  galvanized steel, length 300 mm, mesh width 30/16  mm, load class B 125delivery and installation according to manufacturer’s installation instructionsManufacturer: BIRCO GmbH | **Unit price** | **Total price** |
| **BIRCOplus NW 100 – Outfall unit 19/19** + PP odour trap+ Length 230 mm+ Width 230 mmmade of concrete C 40/50, up to load class A 15 according to EN 1433, PP silt bucket[ ] \_\_\_\_\_ pce. outfall unit, one-piece, construction height 205 mm, integrated socket for DN 100 pipe connection, with ductile iron grating[ ] \_\_\_\_\_ pce. outfall unit, one-piece, construction height 205 mm, integrated socket for DN 100 pipe connection, with mesh gratingdelivery and installation according to manufacturer’s installation instructionsManufacturer: BIRCO GmbH | **Unit price** | **Total price** |
| **BIRCOplus NW 100 – Cutting of channels including grating** and painting or galvanizing of cut angles and gratings. For mesh gratings welding of end pieces and galvanizing. [ ] \_\_\_\_\_ 90° cut[ ] \_\_\_\_\_ Mitre cut according to degree specificationManufacturer: BIRCO GmbH | **Unit price** | **Total price** |
| **BIRCOplus NW 100 – Hole drilling of channel**[ ] \_\_\_\_\_ in horizontal / vertical direction, diameter DN 100[ ] \_\_\_\_\_ pce of silt bucket(s)delivery.Manufacturer: BIRCO GmbH | **Unit price** | **Total price** |