|  |  |  |
| --- | --- | --- |
| **BIRCOsir NW 200 AS – Drainage channel with 0.5 % inbuilt fall** with integrated two-sided anchoring system (AS) made of concrete  + Length 1000 mm  + Width at angle 300 mm, width at bottom 332 mm  + Construction height at groove/tongue 310 to 360 mm  made of concrete C 40/50 according to EN 1433, up to load class D 400 Type I / F 900 Type M as defined by EN 1433, with anchored 4 mm hot-dipped galvanized solid steel angles for combi-closure system (70 µm zinc coating), with safety sealing joint  [ ] \_\_\_\_\_ m BIRCOsir NW 200 AS channel No. 1 – 10  [ ] Sealing with SF-Connect  including necessary end caps, delivery and installation according to manufacturer’s installation instructions.  Manufacturer:  BIRCO GmbH Herrenpfädel 142, D 76532 Baden-Baden Phone +497221 - 5003-0; Fax +497221 - 5003-1149; www.birco.de | **Unit price** | **Total price** |
| **BIRCOsir NW 200 AS – – Drainage channel without inbuilt fall** with integrated two-sided anchoring system (AS) made of concrete  + Length 500 mm (just height 310 mm)/1000 mm  + Width at angle 300 mm, width at bottom 332 mm  + Construction height 310/335/360/410 mm  made of concrete C 40/50 according to EN 1433, up to load class D 400 Type I / F 900 Type M as defined by EN 1433, with anchored 4 mm hot-dipped galvanized solid steel angles for combi-closure system (70 µm zinc coating), with safety sealing joint  [ ] \_\_\_\_\_ m BIRCOsir NW 200 AS channel No. 0/0, 5/0, 10/0,   20/0  [ ] Sealing with SF-Connect  including necessary end caps, delivery and installation according to manufacturer’s installation instructions.  Manufacturer: BIRCO GmbH | **Unit price** | **Total price** |

|  |  |  |
| --- | --- | --- |
| **BIRCOsir NW 200 AS – Shallow channel without inbuilt fall** with integrated two-sided anchoring system (AS) made of concrete  + Length 1000 mm  + Width at angle 300 mm, width at bottom 334 mm  + Construction height 200 / 250 mm  made of concrete C 40/50 according to EN 1433, up to load class E 600 as defined by EN 1433, with anchored 4 mm hot-dipped galvanized solid steel angles for combi-closure system (70 µm zinc coating), with safety sealing joint  [ ] \_\_\_\_\_ m BIRCOsir NW 200 AS shallow channel construction   height 200/250  [ ] Sealing with SF-Connect  including necessary end caps, delivery and installation according to manufacturer’s installation instructions.  Manufacturer: BIRCO GmbH | **Unit price** | **Total price** |
| **BIRCOsir NW 200 AS – End caps and end caps with outlet DN 200**  + Width 330 mm  made of galvanized steel  [ ] \_\_\_\_\_ pce. of end cap(s) for channel no. 0/0–5/0 / 6–10/0 / 20/0  [ ] \_\_\_\_\_ pce. of end cap(s) for shallow channel,   construction height 200 / 250 mm  [ ] \_\_\_\_\_ pce. of end cap(s) with outlet DN 200 for channel   no. 0/0 / 5/0 / 10/0 / 20/0  delivery.  Manufacturer:  BIRCO GmbH | **Unit price** | **Total price** |

|  |  |  |
| --- | --- | --- |
| **BIRCOsir NW 200 AS – – In-line outfall unit** for 1- or 2-sided channel connection,with integrated two-sided anchoring system (AS) made of concrete  + Length at angle 500 mm, Length at bottom 510 mm  + Width at angle 300 mm, width at bottom 345 mm,  + Galvanized silt bucket  + Without odour trap  made of concrete C 40/50 according to EN 1433, up to load class F 900 as defined by EN 1433, with anchored 4 mm hot-dipped galvanized solid steel angles for combi-closure system (70 µm zinc coating), with safety sealing joint  [ ] \_\_\_\_\_ pce in-line outfall unit, 1 piece, construction height   740 mm, integrated socket for DN 200 pipe   connection  [ ] Sealing with SF-Connect  including necessary end caps, delivery and installation according to manufacturer’s installation instructions.  Manufacturer: BIRCO GmbH | **Unit price** | **Total price** |
| **BIRCOsir NW 200 AS – Gratings**  + Width 287 mm  + Height 30 mm  load class according to DIN EN 1433, with 8-point per meter M12/A2-bolt fastening or Easylock fastening, mesh grating  4 point fastening per grating  [ ] \_\_\_\_\_ pce ductile iron slotted grating black immersion-  lacquered, length 500 mm, load class D 400 / E 600 /   F 900  [ ] \_\_\_\_\_ pce ductile iron mesh grating black immersion-  lacquered, length 500 mm, load class C 250 / E 600  [ ] \_\_\_\_\_ pce ductile iron honeycomb gratings black immersion-  lacquered, length 500 mm, load class E 600 / F 900  [ ] \_\_\_\_\_ pce mesh grating galvanized steel,   length 500 / 1000 mm, mesh width 30/30, load class  C 250  delivery and installation according to manufacturer’s installation instructions.  Manufacturer: BIRCO GmbH | **Unit price** | **Total price** |
| **BIRCOsir NW 200 AS – Cutting of channels including grating** and painting or galvanizing of cut angles and gratings. For mesh gratings welding of end pieces and galvanizing.  [ ] \_\_\_\_\_ 90° cut  [ ] \_\_\_\_\_ Mitre cut according to degree specification  Manufacturer: BIRCO GmbH | **Unit price** | **Total price** |

|  |  |  |
| --- | --- | --- |
| **BIRCOsir NW 200 AS – Hole drilling of channel**  [ ] \_\_\_\_\_ in horizontal / vertical direction, diameter DN 200  [ ] \_\_\_\_\_ pce of silt bucket(s)  [ ] \_\_\_\_\_ pce of silt bucket(s) for shallow channels  Delivery.  Manufacturer: BIRCO GmbH | **Unit price** | **Total price** |