|  |  |  |
| --- | --- | --- |
| **BIRCOsir NW 300 AS – Drainage channel with 0.5% inbuilt fall** with integrated two-sided anchoring system (AS) made of concrete  + Length 1000 mm, 2000 mm  + Width at angle 430 mm, width at bottom 470 mm  + Construction height 410 mm to 550 mm  made of concrete C 40/50 according to EN 1433, up to load class D 400 Type I / F 900 Type M as defined by EN 1433, with anchored 4 mm hot-dipped galvanized solid steel angles for combi-closure system (70 µm zinc coating), with safety sealing joint  [ ] \_\_\_\_\_ m BIRCOsir NW 300 AS channel construction   No. 1 - 28, length 1000 / 2000 mm  [ ] Sealing with SF-Connect  including necessary end caps, delivery and installation according to manufacturer’s installation instructions.  Manufacturer:  BIRCO GmbH Herrenpfädel 142, D 76532 Baden-Baden Phone +497221 - 5003-0; Fax +497221 - 5003-1149; www.birco.de | **Unit price** | **Total price** |
| **BIRCOsir NW 300 AS – Drainage channel without inbuilt fall** with integrated two-sided anchoring system (AS) made of concrete  + Length 1000 mm, 2000 mm  + Width at angle 430 mm, width at bottom 470 mm  + Construction height 1: 410 mm/ Construction height 2: 550 mm  made of concrete C 40/50 according to EN 1433, up to load class D 400 Type I / F 900 Type M as defined by EN 1433, with anchored 4 mm hot-dipped galvanized solid steel angles for combi-closure system (70 µm zinc coating), with safety sealing joint  [ ] \_\_\_\_\_ m BIRCOsir NW 300 AS channel construction   height 1 / 2, length 1000 / 2000 mm  [ ] Sealing with SF-Connect  including necessary end caps, delivery and installation according to manufacturer’s installation instructions.  Manufacturer:  BIRCO GmbH Herrenpfädel 142, D 76532 Baden-Baden Phone +497221 - 5003-0; Fax +497221 - 5003-1149; www.birco.de | **Unit price** | **Total price** |

|  |  |  |
| --- | --- | --- |
| **BIRCOsir NW 300 AS – Shallow channel without inbuilt fall** with integrated two-sided anchoring system (AS) made of concrete  + Length 1000 mm  + Width at angle 430 mm, width at bottom 470 mm  + Construction height 300 mm  made of concrete C 40/50 according to EN 1433, up to load class E 600 as defined by EN 1433, with anchored 4 mm hot-dipped galvanized solid steel angles for combi-closure system (70 µm zinc coating), with safety sealing joint  [ ] \_\_\_\_\_ m BIRCOsir NW 300 AS shallow channel  [ ] Sealing with SF-Connect  including necessary end caps, delivery and installation according to manufacturer’s installation instructions.  Manufacturer:  BIRCO GmbH | **Unit price** | **Total price** |
| **BIRCOsir NW 300 AS – End caps and end caps with outlet DN 200**  + Width 430 mm  made of galvanized steel  [ ] \_\_\_\_\_ pce. of end cap(s) for channel construction height 1 / 2  [ ] \_\_\_\_\_ pce. of end cap(s) for shallow channel  [ ] \_\_\_\_\_ pce. of end cap(s) with outlet DN 200 for channel   construction height 1 / 2  delivery.  Manufacturer: BIRCO GmbH | **Unit price** | **Total price** |
| **BIRCOsir NW 300 AS – In-line outfall unit** for 1- or 2-sided channel connection,with integrated two-sided anchoring system (AS) made of concrete  + Length 500 m  + Width at angle 430 mm, width at bottom 460mm  + Galvanized silt bucket  + Integrated socket for DN 300 pipe connection  + Without odour trap  made of concrete C 40/50 according to EN 1433, up to load class F 900 as defined by EN 1433, with anchored 4 mm hot-dipped galvanized solid steel angles for combi-closure system (70 µm zinc coating), with safety sealing joint  [ ] \_\_\_\_\_ pce in-line outfall unit, 1 piece, construction height   980 mm  [ ] Sealing with SF-Connect  including necessary end caps, delivery and installation according to manufacturer’s installation instructions.  Manufacturer:  BIRCO GmbH | **Unit price** | **Total price** |

|  |  |  |
| --- | --- | --- |
| **BIRCOsir NW 300 AS – Gratings**  + Width 417 mm  + Height 35 mm  load class according to DIN EN 1433, with 8-point per meter M12/A2-bolt fastening or Easylock fastening, mesh grating  4 point fastening per grating  [ ] \_\_\_\_\_ pce ductile iron twofold slotted grating black   immersion- lacquered, length 500 mm,   load class D 400 / E 600 / F 900  [ ] \_\_\_\_\_ pce ductile iron mesh grating black immersion-  lacquered, length 500 mm, load class C 250 / E 600 [ ] \_\_\_\_\_ pce bulb ducitile iron cover, black immersion-  lacquered, length 500 mm, load class E 600  delivery and installation according to manufacturer’s installation instructions.  Manufacturer:  BIRCO GmbH | **Unit price** | **Total price** |
| **BIRCOsir NW 300 AS – Cutting of channels including grating** and painting or galvanizing of cut angles and gratings. For mesh gratings welding of end pieces and galvanizing.  [ ] \_\_\_\_\_ 90° cut  [ ] \_\_\_\_\_ Mitre cut according to degree specification  Manufacturer: BIRCO GmbH | **Unit price** | **Total price** |
| **BIRCOsir NW 300 AS – Hole drilling of channel**  [ ] \_\_\_\_\_ in horizontal / vertical direction, diameter DN 300  [ ] \_\_\_\_\_ pce of silt bucket(s)  [ ] \_\_\_\_\_ pce of silt bucket(s) for shallow channels  Delivery.  BIRCO GmbH | **Unit price** | **Total price** |