|  |  |  |
| --- | --- | --- |
| **BIRCOsir Point Drainage 30/30 – Outfall unit** alsofor drainage channel connection on two sides (NW 100)  + Length at angle frame 300 mm/ Length at bottom 320 mm  + Width at angle frame 300 mm/ Width at bottom 320 mm  + PP odour trap  + PP silt bucket  + Integrated socket for DN 100 pipe connection  made of concrete C 40/50 according to EN 1433, up to load class E 600 as defined by EN 1433, with anchored 4 mm hot-dipped galvanized solid steel angles for combi-closure system (70 µm zinc coating), with safety sealing joint  [ ] \_\_\_\_\_ pce outfall unit, 1 piece, construction height 420 mm  [ ] Sealing with SF-Connect  including necessary end caps, delivery and installation according to manufacturer’s installation instructions.  Manufacturer: BIRCO GmbH Herrenpfädel 142, D 76532 Baden-Baden Phone +497221 - 5003-0; Fax +497221 - 5003-1149; www.birco.de | **Unit price** | **Total price** |
| **BIRCOsir Point Drainage 30/30 – Gratings**  + Width 280 mm  + Height 30 mm  load class according to DIN EN 1433, with 2-point per grating M12/A2-bolt fastening or Easylock fastening  [ ] \_\_\_\_\_ pce ductile iron twofold slotted grating black   immersion-lacquered, length 280 mm, load class E 600  [ ] \_\_\_\_\_ pce mesh grating galvanized steel,   length 280 mm, mesh width 30/30 mm / 30/15 mm, load class C 250  delivery and installation according to manufacturer’s installation instructions.  Manufacturer: BIRCO GmbH | **Unit price** | **Total price** |

|  |  |  |
| --- | --- | --- |
| **BIRCOsir Point Drainage 40/40 – Outfall unit, 1-piece** alsofor drainage channel connection on three sides (NW 100 and 150)  + Length at angle 400 mm/ Length at bottom 415 mm  + Width at angle frame 400 mm/ Width at bottom 415 mm  + PP odour trap  + PP silt bucket  + Integrated socket for DN 150 pipe connection  made of concrete C 40/50 according to EN 1433, up to load class E 600 as defined by EN 1433, with anchored 4 mm hot-dipped galvanized solid steel angles for combi-closure system (70 µm zinc coating), with safety sealing joint  [ ] \_\_\_\_\_ pce outfall unit, 1 piece, construction height 575 mm  [ ] Sealing with SF-Connect  including necessary end caps, delivery and installation according to manufacturer’s installation instructions.  Manufacturer: BIRCO GmbH Herrenpfädel 142, D 76532 Baden-Baden Phone +497221 - 5003-0; Fax +497221 - 5003-47; www.birco.de | **Unit price** | **Total price** |
| **BIRCOsir Point Drainage 40/40 – outfall unit, 2-piece**  + Length at angle 400 mm/ Length at bottom 410 mm  + Width at angle frame 400 mm/ Width at bottom 410 mm  + PP odour trap  + PP silt bucket  + Integrated socket for DN 200 pipe connection  made of concrete C 40/50 according to EN 1433, up to load class E 600 as defined by EN 1433, with anchored 4 mm hot-dipped galvanized solid steel angles for combi-closure system (70 µm zinc coating), with safety sealing joint  [ ] \_\_\_\_\_ pce outfall unit, 2-piece, construction height 880 mm  including necessary end caps, delivery and installation according to manufacturer’s installation instructions.  Manufacturer: BIRCO GmbH | **Unit price** | **Total price** |

|  |  |  |
| --- | --- | --- |
| **BIRCOsir Point Drainage 40/40 – outfall unit, 3-piece**  alsofor drainage channel connection on four sides (NW 100, NW 150, NW 200 to no. 20)  + Length at angle 400 mm / Length at bottom 410 mm  + Width at angle frame 400 mm/ Width at bottom 410 mm  + PP odour trap  + PP silt bucket  + Integrated socket for DN 200 pipe connection  made of concrete C 40/50 according to EN 1433, up to load class E 600 as defined by EN 1433, with anchored 4 mm hot-dipped galvanized solid steel angles for combi-closure system (70 µm zinc coating), with safety sealing joint  [ ] \_\_\_\_\_ pce outfall unit, 3-piece, construction height 1200 mm  including necessary end caps, delivery and installation according to manufacturer’s installation instructions.  Manufacturer: BIRCO GmbH | **Unit price** | **Total price** |
| **BIRCOsir Point Drainage 40/40 – Gratings**  + Width 380 mm  + Height 40 mm  load class according to DIN EN 1433, with 4-point per grating M12/A2-bolt fastening or Easylock fastening  [ ] \_\_\_\_\_ pce ductile iron twofold slotted grating black immersion-  lacquered, length 380 mm, load class E 600  [ ] \_\_\_\_\_ pce mesh grating galvanized steel,   length 380 mm,   mesh width 30/30, load class C 250  mesh width 30/15, load class C 250  mesh width 20/30, load class E 600  delivery and installation according to manufacturer’s installation instructions.  Manufacturer: BIRCO GmbH | **Unit price** | **Total price** |