|  |  |  |
| --- | --- | --- |
| **BIRCOsir Rail track drainage rail profile 49E1/54E3 (old designation: S 49/S 54)**+ Channel BIRCOsir NW 100, no. 0/0+ 2-piece+ Two-sided rail track drainage casings for collecting surface  water+ Ductile iron slotted grating black immersion-lacquered+ 8-point per metre M12/A2-bolt fastening + Integrated sockets for DN 100 pipe connection DN 100[ ] \_\_\_\_\_ pce tail track drainage, gauge 1435 mm,  construction height 180 mm[ ] Sealing with SF-Connectdelivery and installation according to manufacturer’s installation instructions.Manufacturer: BIRCO GmbHHerrenpfädel 142, D 76532 Baden-BadenPhone +497221 - 5003-0; Fax +497221 - 5003-1149; www.birco.de | **Unit price** | **Total price** |
| **BIRCOsir Rail track drainage rail profile 57R1/67R1 (old designation: Ph37/Ph37a)**+ Channel BIRCOsir NW 100, no. 0/0+ 3-piece+ Two-sided rail track drainage casings for collecting surface  water+ Ductile iron slotted grating black immersion-lacquered+ 8-point per metre M12/A2-bolt fastening+ Integrated sockets for DN 100 pipe connection DN 100[ ] \_\_\_\_\_ pce tail track drainage, gauge 1435 mm construction height 180 mm[ ] Sealing with SF-Connectdelivery and installation according to manufacturer’s installation instructions.Manufacturer: BIRCO GmbHHerrenpfädel 142, D 76532 Baden-BadenPhone +497221 - 5003-0; Fax +497221 - 5003-47; www.birco.de | **Unit price** | **Total price** |