|  |  |  |
| --- | --- | --- |
| **BIRCOslot channel Pfuhler DN 200 – channel element type I without inbuilt fall, ASR resistant**  + Monolithic concrete body  + Length 4000 mm  + Width at top 370 mm, width at bottom 400 mm  + Construction height 400 mm  + Cross sectional area: 314 cm²  made of concrete C 40/50 according to EN 1433, up to load class as defined by EN 1433  [ ] \_\_\_\_\_ m BIRCOslot channel Pfuhler DN 200, load class D 400,   intermittent slot, slot width 30/50 mm, inclined surface   to the slot  [ ] \_\_\_\_\_ m BIRCOslot channel Pfuhler DN 200, load class D 400,   continuous slot, slot width 30/50 mm, inclined surface   to the slot  [ ] \_\_\_\_\_ m BIRCOslot channel Pfuhler DN 200, load class F 900,   intermittent slot, slot width 30/50 mm,   plane surface  [ ] \_\_\_\_\_ m BIRCOslot channel Pfuhler DN 200, load class D 400   / F 900, length \_\_\_\_\_\_\_ mm (between 250 and 3950   mm, to enquire about)  [ ] Channel with integrated kerb  [ ] Sealing with lubricant DENSO  delivery and installation according to manufacturer’s installation instructions.  Manufacturer:  BIRCO GmbH Herrenpfädel 142, D 76532 Baden-Baden Phone +497221 - 5003-0; Fax +497221 - 5003-1149; www.birco.de | **Unit price** | **Total price** |

|  |  |  |
| --- | --- | --- |
| **BIRCOslot channel Pfuhler DN 200 – channel element with outlet, type I, ASR resistant**  + Monolithic concrete body  + Length 1000 mm  + Width at top 370 mm  + Total height 1000 mm  made of concrete C 40/50 according to EN 1433, up to load class as defined by EN 1433  Channel element with vertical outlet DN 200, silk bucket and ductile iron grating  [ ] \_\_\_\_\_ pce BIRCOslot channel element with outlet Pfuhler   DN 200, load class D 400, with inclined surface the slot  [ ] \_\_\_\_\_ pce BIRCOslot channel element with outlet Pfuhler   DN 200, load class F 900, with plane surface  [ ] Sealing with lubricant DENSO  delivery and installation according to manufacturer’s installation instructions.  Manufacturer:  BIRCO GmbH | **Unit price** | **Total price** |
| **BIRCOslot channel Pfuhler DN 200 – inspection channel, type I without inbuilt fall, ASR resistant**  + Monolithic concrete body  + Length 1000 mm  + Width at top 370 mm, width at ground 400 mm  + Total height 400  made of concrete C 40/50 according to EN 1433, up to load class as defined by EN 1433 and ductile iron grating  [ ] \_\_\_\_\_ pce inspection channel Pfuhler DN 200, load class   D 400, with inclined surface the slot  [ ] \_\_\_\_\_ pce inspection channel Pfuhler DN 200, load class   F 900, with plane surface  [ ] Sealing with lubricant DENSO  delivery and installation according to manufacturer’s installation instructions.  Manufacturer:  BIRCO GmbH | **Unit price** | **Total price** |
| **BIRCOslot channel Pfuhler DN 200 – end cap**  Made of galvanized steel  [ ] \_\_\_\_\_ pce of end cap, construction height 400 mm  delivery.  Manufacturer:  BIRCO GmbH | **Unit price** | **Total price** |