|  |  |  |
| --- | --- | --- |
| **BIRCOslot channel Pfuhler DN 300 – channel element type I without inbuilt fall, ASR resistant**  + Monolithic concrete body  + Length 4000 mm  + Width at top 460 mm, width at bottom 500 mm  + Construction height 500 mm  + Cross sectional area: 706 cm²  made of concrete C 40/50 according to EN 1433, up to load class as defined by EN 1433  [ ] \_\_\_\_\_ m BIRCOslot channel Pfuhler DN 300, load   class D 400, intermittent slot, slot width 30/50 mm,   inclined surface to the slot  [ ] \_\_\_\_\_ m BIRCOslot channel Pfuhler DN 300, load   class D 400, continuous slot, slot width 30/50 mm,   inclined surface to the slot  [ ] \_\_\_\_\_ m BIRCOslot channel Pfuhler DN 300, load   class F 900, intermittent slot, slot width 30/50 mm,   plane surface  [ ] \_\_\_\_\_ m BIRCOslot channel Pfuhler DN 300, load   class D 400 / F 900, length \_\_\_\_\_\_\_ mm (between 250   and 3950 mm, to enquire about)  [ ] Channel with integrated kerb  [ ] Sealing with lubricant DENSO  delivery and installation according to manufacturer’s installation instructions.  Manufacturer:  BIRCO GmbH Herrenpfädel 142, D 76532 Baden-Baden Phone +497221 - 5003-0; Fax +497221 - 5003-1149; www.birco.de | **Unit price** | **Total price** |

|  |  |  |
| --- | --- | --- |
| **BIRCOslot channel Pfuhler DN 300 – channel element type I with inbuilt fall, ASR resistant**  + Monolithic concrete body  + Length 4000 mm  + Width at top 460 mm, width at bottom 500 mm  + Construction height 500 mm  + Cross sectional area: 555 to 706 cm²  made of concrete C 40/50 according to EN 1433, up to load class as defined by EN 1433  [ ] \_\_\_\_\_ m BIRCOslot channel Pfuhler DN 300, channel   no. 1-5, load class D 400, intermittent slot, slot width   30/50 mm, inclined surface to the slot  [ ] \_\_\_\_\_ m BIRCOslot channel Pfuhler DN 300, channel   no. 1-5, load class D 400, continuous slot, slot width   30/50 mm, inclined surface to the slot  [ ] \_\_\_\_\_ m BIRCOslot channel Pfuhler DN 300, channel   no. 1-5, load class F 900, intermittent slot, slot width   30/50 mm, plane surface  [ ] \_\_\_\_\_ m BIRCOslot channel Pfuhler DN 300, channel   no. 1-5, load class D 400 / F 900, length \_\_\_\_\_\_\_   mm (between 250 and 3950 mm, to enquire about)  [ ] Channel with integrated kerb  [ ] Sealing with lubricant DENSO  delivery and installation according to manufacturer’s installation instructions.  Manufacturer:  BIRCO GmbH | **Unit price** | **Total price** |

|  |  |  |
| --- | --- | --- |
| **BIRCOslot channel Pfuhler DN 300 – channel element with outlet, type I, ASR resistant**  + Monolithic concrete body  + Length 1000 mm  + Width at top 460 mm  + Total height 1210 mm  made of concrete C 40/50 according to EN 1433, up to load class as defined by EN 1433  Channel element with vertical outlet DN 300, silk bucket and ductile iron grating  [ ] \_\_\_\_\_ pce BIRCOslot channel element with outlet Pfuhler   DN 300, load class D 400, with inclined surface   the slot  [ ] \_\_\_\_\_ pce BIRCOslot channel element with outlet Pfuhler   DN 300, load class F 900, with plane surface  [ ] Sealing with lubricant DENSO  delivery and installation according to manufacturer’s installation instructions.  Manufacturer:  BIRCO GmbH | **Unit price** | **Total price** |
| **BIRCOslot channel Pfuhler DN 300 – inspection channel, type I without inbuilt fall, ASR resistant**  + Monolithic concrete body  + Length 1000 mm  + Width at top 460 mm, width at ground 500 mm  + Total height 500 mm  made of concrete C 40/50 according to EN 1433, up to load class as defined by EN 1433 and ductile iron grating  [ ] \_\_\_\_\_ pce inspection channel Pfuhler DN 300, load   class D 400, with inclined surface the slot  [ ] \_\_\_\_\_ pce inspection channel Pfuhler DN 300, load   class F 900, with plane surface  [ ] Sealing with lubricant DENSO  delivery and installation according to manufacturer’s installation instructions.  Manufacturer:  BIRCO GmbH | **Unit price** | **Total price** |
| **BIRCOslot channel Pfuhler DN 300 – end cap**  + for channels without inbuilt fall  Made of galvanized steel  [ ] \_\_\_\_\_ pce of end cap, construction height 500 mm  delivery.  Manufacturer:  BIRCO GmbH | **Unit price** | **Total price** |

|  |  |  |
| --- | --- | --- |
| **BIRCOslot channel Pfuhler DN 300 – end cap**  + for channels with inbuilt fall  Made of concrete  [ ] \_\_\_\_\_ pce of end cap female, construction height 500 mm  [ ] \_\_\_\_\_ pce of end cap male, construction height 500 mm  delivery.  Manufacturer:  BIRCO GmbH | **Unit price** | **Total price** |