|  |  |  |
| --- | --- | --- |
| **BIRCOslot steel tops NW 150 AS - material thickness  4 mm**  + For channel elements NW 150 AS  + Length 500 mm / 1000 mm  + Width 210 mm  + Total height 174/ 204 mm  made of galvanized steel, up to load class E 600 as defined by EN 1433  [ ] \_\_\_\_\_ pce. symmetrical BIRCOslot steel top NW 150 AS   neck height 170 mm, length 500 / 1000 mm  [ ] \_\_\_\_\_ pce. symmetrical BIRCOslot steel top NW 150 AS   neck height 200 mm, length 500 / 1000 mm  [ ] \_\_\_\_\_ pce assymetrical BIRCOslot steel top NW 150 AS   neck height 134 mm, length 500 / 1000 mm  [ ] \_\_\_\_\_ pce assymetrical BIRCOslot steel top NW 150 AS   neck height 165 mm, length 500 / 1000 mm  delivery and installation according to manufacturer’s installation instructions.  Manufacturer:  BIRCO GmbH Herrenpfädel 142, D 76532 Baden-Baden Phone +497221 - 5003-0; Fax +497221 - 5003-1149; www.birco.de | **Unit price** | **Total price** |
| **BIRCOslot steel tops NW 150 AS – access top two-piece material thickness 4 mm**  + For channel elements / outfall units  + with removable insert as maintenance and cleaning aperture  + Length 500 mm  + Width 210 mm  + For total height 174/204 mm  made of galvanized steel, up to load class E 600 as defined by EN 1433  [ ] \_\_\_\_\_ access top with symmetrical slot, total height 174 mm  [ ] \_\_\_\_\_ access top with symmetrical slot, total height 204 mm  [ ] \_\_\_\_\_ access top with asymmetrical slot, total height 174 mm  [ ] \_\_\_\_\_ access top with asymmetrical slot, total height 204 mm  delivery and installation according to manufacturer’s installation instructions.  Manufacturer:  BIRCO GmbH | **Unit price** | **Total price** |

|  |  |  |
| --- | --- | --- |
| **BIRCOslot steel tops NW 150 AS - material thickness  1,5 mm**  + For channel elements  + Length 500 mm / 1000 mm,  + Width 212 mm  + Total height 151,5/201,5 mm  made of galvanized steel, up to load class C 250 as defined by EN 1433  [ ] \_\_\_\_\_ pce. symmetrical BIRCOslot steel top NW 150 AS,  neck height 150 mm, length 500 / 1000 mm  [ ] \_\_\_\_\_ pce. symmetrical BIRCOslot steel top NW 150 AS,  neck height 200 mm, length 500 / 1000 mm  [ ] \_\_\_\_\_ pce. asymmetrical BIRCOslot steel top NW 150 AS,   neck height 126 mm, length 500 / 1000 mm  [ ] \_\_\_\_\_ pce. asymmetrical BIRCOslot steel top NW 150 AS,   neck height 180 mm, length 500 / 1000 mm  delivery and installation according to manufacturer’s installation instructions.  Manufacturer:  BIRCO GmbH Herrenpfädel 142, D 76532 Baden-Baden Phone +497221 - 5003-0; Fax +497221 - 5003-1149; www.birco.de | **Unit price** | **Total price** |
| **BIRCOslot steel tops NW 150 AS – access top two-piece material thickness 1,5 mm**  + For channel elements / outfall units  + With removable insert as maintenance and cleaning aperture  + Length 500 mm  + Width 212 mm  + For total height 151,5/201,5 mm  made of galvanized steel  [ ] \_\_\_\_\_ access top with symmetrical slot,  total height 151,5 mm  [ ] \_\_\_\_\_ access top with symmetrical slot,  total height 201,5 mm  [ ] \_\_\_\_\_ access top with asymmetrical slot,  total height 151,5 mm  [ ] \_\_\_\_\_ access top with asymmetrical slot,  total height 201,5 mm  delivery and installation according to manufacturer’s installation instructions.  Manufacturer: BIRCO GmbH | **Unit price** | **Total price** |

|  |  |  |
| --- | --- | --- |
| **BIRCOslot steel tops NW 150 AS – Drainage channel without inbuilt fall**  + Length 500 mm (just for height 205 mm)/1000 mm  + Width at top 212 mm, width at bottom 244 mm  + Construction height at groove/tongue 205 to 300 mm  + Concrete edge protected by slot steel top / access top  made of concrete C 40/50 according to EN 1433, up to load class E 600 as defined by EN 1433, with safety sealing joint  [ ] \_\_\_\_\_ m BIRCOslot steel top NW 150 AS channel no. 0/0,   5/0, 10/0, 20/0  [ ] Sealing with SF-Connect  including necessary end caps, delivery and installation according to manufacturer’s installation instructions.  Manufacturer: BIRCO GmbH | **Unit price** | **Total price** |
| **BIRCOslot steel tops NW 150 AS – outfall unit** for 1- or 2-sided channel connection  + PP odour trap  + PP silt bucket  + Integrated socket for DN 100 pipe connection DN 150  + Length 500 mm  + Width 212 mm  + Concrete edge protected by slot steel top / access top  made of concrete C 40/50 according to EN 1433, up to load class E 600 as defined by EN 1433,  [ ] \_\_\_\_\_ pce outfall unit, one piece, construction height 685 mm  including necessary end caps, delivery and installation according to manufacturer’s installation instructions.  Manufacturer: BIRCO GmbH | **Unit price** | **Total price** |
| **BIRCOslot steel tops NW 150 AS – End caps**  + Galvanized steel  [ ] \_\_\_\_\_ pce end caps for no. 0/0-4 / 5/0-8 / 9-10 / 20/0  delivery.  Manufacturer:  BIRCO GmbH | **Unit price** | **Total price** |
| **BIRCOslot steel tops NW 150 AS – Lifting device for access top**  [ ] \_\_\_\_\_ pce lifting device  delivery.  Manufacturer:  BIRCO GmbH | **Unit price** | **Total price** |

|  |  |  |
| --- | --- | --- |
| **BIRCOslot steel tops NW 150 AS – Cutting of channel with slot steel top** and galvanizing of the top  [ ] \_\_\_\_\_ Channel section 90°  [ ] \_\_\_\_\_ Mitre cut according to degree specification  Manufacturer:  BIRCO GmbH | **Unit price** | **Total price** |
| **BIRCOslot steel tops NW 150 AS – Hole drilling of channel**  [ ] \_\_\_\_\_ in horizontal / vertical direction, diameter DN 150  delivery.  Manufacturer:  BIRCO GmbH | **Unit price** | **Total price** |