|  |  |  |
| --- | --- | --- |
| **BIRCOtop F 100 Series without visible edge – Drainage channel**  + Perforated on one side  + Bolt connection bar  + Length 500 / 1000 / 3000 mm  + Width 100 mm  + Construction height 50 / 75 / 100 mm  made of galvanized steel  [ ] \_\_\_\_\_ pce BIRCOtop F 100, channel construction height   50/75/100, load class walkable, length 500/1000/3000   mm  delivery and installation according to manufacturer’s installation instructions.  Manufacturer:  BIRCO GmbH Herrenpfädel 142, D 76532 Baden-Baden Phone +497221 - 5003-0; Fax +497221 - 5003-1149; www.birco.de | **Unit price** | **Total price** |
| **BIRCOtop F 100 Series – End caps**  + Width 100 mm  + For construction height 50 / 75 / 100 mm  made of galvanized steel  [ ] \_\_\_\_\_ pce BIRCOtop F 100 end cap for construction height   50/75/100  delivery and installation according to manufacturers installation instructions.  Manufacturer:  BIRCO GmbH | **Unit price** | **Total price** |

|  |  |  |
| --- | --- | --- |
| **BIRCOtop F 100 Series – Gratings**  + Width 92 mm  + Height 20 mm  With 2-point per meter M10/A2 bolt connection  [ ] \_\_\_\_\_ pce punched hole grating – circular holes, made of hot-  dipped galvanized steel, length 500 / 1000 mm,   load class walkable  [ ] \_\_\_\_\_ pce punched hole grating – square holes, made of hot-  dipped galvanized steel, length 500 / 1000 mm,   load class walkable  [ ] \_\_\_\_\_ pce slot grating made of hot-dipped galvanized steel,   length 500 / 1000 mm, load class walkable  [ ] \_\_\_\_\_ pce longitudinal bar grating made of hot-dipped   galvanized steel, length 500 / 1000 mm, load class   walkable  [ ] \_\_\_\_\_ pce mesh grating made of hot-dipped galvanized steel,   length 500 / 1000 mm, mesh width 30/10  load class walkable  delivery and installation according to manufacturers installation instructions.  Manufacturer:  BIRCO GmbH | **Unit price** | **Total price** |