|  |  |  |
| --- | --- | --- |
| **BIRCOtop F 130 Series without visible edge – Drainage channel**+ Perforated on one side+ Bolt connection bar+ Length 500 / 1000 / 3000 mm + Width 130 mm+ Construction height 50 / 75 / 100 mmmade of galvanized steel[ ] \_\_\_\_\_ pce BIRCOtop F 130, channel construction 50/75/100, length 500/1000/3000 mm, load class walkabledelivery and installation according to manufacturer’s installation instructions.Manufacturer: BIRCO GmbHHerrenpfädel 142, D 76532 Baden-BadenPhone +497221 - 5003-0; Fax +497221 - 5003-1149; www.birco.de | **Unit price** | **Total price** |
| **BIRCOtop F 130 Series – End caps**+ Width 130 mm+ For construction height 50 / 75 / 100 mmmade of galvanized steel[ ] \_\_\_\_\_ pce BIRCOtop F 130 end cap for construction height  50 / 75 / 100 mmdelivery and installation according to manufacturers installation instructions.Manufacturer: BIRCO GmbH | **Unit price** | **Total price** |

|  |  |  |
| --- | --- | --- |
| **BIRCOtop F 130 Series – Gratings**+ Width 122 mm+ Height 20 mmWith 2-point per meter M10/A2 bolt connection[ ] \_\_\_\_\_ pce punched hole grating – circular holes, made of hot- dipped galvanized steel, length 500 / 1000 mm,  load class walkable[ ] \_\_\_\_\_ pce punched hole grating – square holes, made of hot- dipped galvanized steel, length 500 / 1000 mm,  load class walkable[ ] \_\_\_\_\_ pce slot grating made of hot-dipped galvanized steel,  length 500 / 1000 mm, load class walkable[ ] \_\_\_\_\_ pce longitudinal bar grating made of hot-dipped  galvanized steel, length 500 / 1000 mm, load class  walkable[ ] \_\_\_\_\_ pce mesh grating made of hot-dipped galvanized steel,  length 500 / 1000 mm, mesh width 30/10 load class walkabledelivery and installation according to manufacturers installation instructions.Manufacturer: BIRCO GmbH | **Unit price** | **Total price** |

|  |  |  |
| --- | --- | --- |
| **BIRCOtop F 130 Series with visible edge – Drainage channel**+ Perforated on two sides+ Without bolt connection+ Length 500 / 1000 mm + Width 130 mm+ Construction height 50 / 75 mmmade of galvanized steel[ ] \_\_\_\_\_ pce BIRCOtop F 100, channel construction height  50/75, length 500/1000mm, load class walkabledelivery and installation according to manufacturer’s installation instructions.Manufacturer: BIRCO GmbHHerrenpfädel 142, D 76532 Baden-BadenPhone +497221 - 5003-0; Fax +497221 - 5003-47; www.birco.de | **Unit price** | **Total price** |
| **BIRCOtop F 130 Series - End caps**+ Width 100 mm+ For construction height 50 / 75 mmmade of galvanized steel[ ] \_\_\_\_\_ pce BIRCOtop F 100 end cap for construction height  50/75 mmdelivery and installation according to manufacturers installation instructions.Manufacturer: BIRCO GmbH | **Unit price** | **Total price** |
| **BIRCOtop F 130 Series – Gratings**+ Width 130 mm[ ] \_\_\_\_\_ pce slot grating made of hot-dipped galvanized steel,  length 500 / 1000 mm, load class walkable[ ] \_\_\_\_\_ pce mesh grating 30/10 made of hot-dipped galvanized  steel, length 500 / 1000 mm, load class walkableinstructions.Manufacturer:BIRCO GmbH | **Unit price** | **Total price** |