|  |  |  |
| --- | --- | --- |
| **BIRCOtop F 160 Series without visible edge – Drainage channel**+ Perforated on one side+ Bolt connection bar+ Length 500 / 1000 / 3000 mm + Width at top 160, at bottom 136 mm+ Construction height 50 / 75 mmmade of galvanized steel[ ] \_\_\_\_\_ pce BIRCOtop F 160, channel construction 50/75 length 500/1000/3000 mm, load class walkabledelivery and installation according to manufacturer’s installation instructions.Manufacturer: BIRCO GmbHHerrenpfädel 142, D 76532 Baden-BadenPhone +497221 - 5003-0; Fax +497221 - 5003-1149; www.birco.de | **Unit price** | **Total price** |
| **BIRCOtop F 160 Series – End caps**+ Width 100 mm+ For construction height 50 / 75 mmmade of galvanized steel[ ] \_\_\_\_\_ pce BIRCOtop F 130 end cap for construction height  50 / 75 mmdelivery and installation according to manufacturers installation instructions.Manufacturer: BIRCO GmbH | **Unit price** | **Total price** |
| **BIRCOtop F 160 Series – Grating**+ Width 153 mm+ Height 20 mmWith 2-point per metre M12/A2 bolt connection [ ] \_\_\_\_\_ pce mesh grating made of hot-dipped galvanized steel,  length 500 / 1000 mm, mesh width 30/10, load class  walkabledelivery and installation according to manufacturers installation instructions.Manufacturer: BIRCO GmbH | **Unit price** | **Total price** |

|  |  |  |
| --- | --- | --- |
| **BIRCOtop F 160 Series with visible edge – Drainage channel**+ Perforated on two sides+ With and without out bolt connection+ Length 500 / 1000 / 3000 mm + Width at top 160 mm, width at bottom 100 mm+ Construction height 50 / 75 / 100 mmmade of galvanized steel[ ] \_\_\_\_\_ pce BIRCOtop F 160, channel construction height  50/75/100 with bolt connection, load class walkable[ ] \_\_\_\_\_ pce BIRCOtop F 160, channel construction height  50/75/100 without bolt connection, load class walkabledelivery and installation according to manufacturer’s installation instructions.Manufacturer: BIRCO GmbHHerrenpfädel 142, D 76532 Baden-BadenPhone +497221 - 5003-0; Fax +497221 - 5003-1149; www.birco.de | **Unit price** | **Total price** |
| **BIRCOtop F 160 Series - End caps**+ Width 160 mm+ For construction height 50 / 75 / 100 mmmade of galvanized steel[ ] \_\_\_\_\_ pce BIRCOtop F 160 end cap for construction height  50/75/100 mmdelivery and installation according to manufacturers installation instructions.Manufacturer:BIRCO GmbH | **Unit price** | **Total price** |
| **BIRCOtop F 160 Series– Gratings**+ Width 158 mm+ Height 20 mm[ ] \_\_\_\_\_ pce slot grating made of hot-dipped  galvanized steel, clamped grating without bolt  connection, length 500 / 1000 mm,  load class walkable[ ] \_\_\_\_\_ pce ductile iron slot grating with 2-point per meter  M10/A2 bolt connection, length 500 mm, load class  walkable[ ] \_\_\_\_\_ pce mesh grating made of hot-dipped galvanized steel,  clamped grating without bolt connection length 500 / 1000 mm, mesh width 30/10 / 30/16 load class walkabledelivery and installation according to manufacturers installation instructions.Manufacturer:BIRCO GmbH | **Unit price** | **Total price** |