|  |  |  |
| --- | --- | --- |
| **BIRCOtop S Series – Drainage channel**  + Not perforated or perforated on one side  + Including removable grate with rectangular punch holes  + Length 3000 mm  + Width at top 20 mm, at bottom 80 mm  + Construction height 150 mm  made of stainless steel (V2A)  [ ] \_\_\_\_\_ pce BIRCOtop S channel load class walkable  delivery and installation according to manufacturer’s installation instructions.  Manufacturer:  BIRCO GmbH Herrenpfädel 142, D 76532 Baden-Baden Phone +497221 - 5003-0; Fax +497221 - 5003-1149; www.birco.de | **Unit price** | **Total price** |
| **BIRCOtop Series S – End caps and connection shoe**  + Width 80 mm  + Construction height 150 mm  made of stainless steel (V2A)  [ ] \_\_\_\_\_ pce. BIRCOtop S end cap right / left  [ ] \_\_\_\_\_ pce BIRCOtop S connection shoe height 55 mm  delivery and installation according to manufacturer’s installation instructions.  Manufacturer:  BIRCO GmbH | **Unit price** | **Total price** |
| **BIRCOtop Series S – Maintenance chamber**  + Wdth 300 mm  + horizontal or vertical outlet DN 100  made of stainless steel (V2A)  [ ] \_\_\_\_\_ pce. maintenance chamber,   length 300 mm, load class walkable  delivery and installation according to manufacturer’s installation instructions.  Manufacturer:  BIRCO GmbH | **Unit price** | **Total price** |