|  |  |  |
| --- | --- | --- |
| **BIRCOtop S Series – Drainage channel**+ Not perforated or perforated on one side+ Including removable grate with rectangular punch holes+ Length 3000 mm + Width at top 20 mm, at bottom 80 mm+ Construction height 150 mmmade of stainless steel (V2A)[ ] \_\_\_\_\_ pce BIRCOtop S channel load class walkabledelivery and installation according to manufacturer’s installation instructions.Manufacturer: BIRCO GmbHHerrenpfädel 142, D 76532 Baden-BadenPhone +497221 - 5003-0; Fax +497221 - 5003-1149; www.birco.de | **Unit price** | **Total price** |
| **BIRCOtop Series S – End caps and connection shoe**+ Width 80 mm+ Construction height 150 mmmade of stainless steel (V2A)[ ] \_\_\_\_\_ pce. BIRCOtop S end cap right / left[ ] \_\_\_\_\_ pce BIRCOtop S connection shoe height 55 mmdelivery and installation according to manufacturer’s installation instructions.Manufacturer: BIRCO GmbH | **Unit price** | **Total price** |
| **BIRCOtop Series S – Maintenance chamber**+ Wdth 300 mm+ horizontal or vertical outlet DN 100made of stainless steel (V2A)[ ] \_\_\_\_\_ pce. maintenance chamber,  length 300 mm, load class walkabledelivery and installation according to manufacturer’s installation instructions.Manufacturer: BIRCO GmbH | **Unit price** | **Total price** |