|  |  |  |
| --- | --- | --- |
| **BIRCOtop attachment elements 40 x 40**  + Circumferential perforation  + Length 250 mm  + Width 250 mm  + Construction height adjustable on-site 59 to 170 mm  made of galvanized steel  [ ] \_\_\_\_\_ pce BIRCOtop attachment element 40 x 40   construction height 59-83 / 82-117 / 115-170,   load class walkable  delivery and installation according to manufacturer’s installation instructions.  Manufacturer:  BIRCO GmbH Herrenpfädel 142, D 76532 Baden-Baden Phone +497221 - 5003-0; Fax +497221 - 5003-1149; www.birco.de | **Unit price** | **Total price** |
| **BIRCOtop accessories 40 x 40 – Gratings**  + Width 392 mm  + Length 392 mm  + Height 20 mm  with 1-point M10/A2 bolt connection  [ ] \_\_\_\_\_ pce punched hole grating – circular holes, made of hot-  dipped galvanized steel, load class walkable  [ ] \_\_\_\_\_ pce slot grating made of hot-dipped galvanized steel,   load class walkable  [ ] \_\_\_\_\_ pce mesh grating made of hot-dipped galvanized steel,   mesh width 30/10, load class walkable  delivery and installation according to manufacturer’s installation instructions.  Manufacturer: BIRCO GmbH | **Unit price** | **Total price** |
| **BIRCOtop – Branch channel**  + Perforated on both sides  + Width 100 mm, length 2000 mm  + Height 30 mm  [ ] \_\_\_\_\_ pce branch channel made of hot-dipped galvanized   steel, load class walkable  delivery and installation according to manufacturer’s installation instructions.  Manufacturer: BIRCO GmbH | **Unit price** | **Total price** |