|  |  |  |
| --- | --- | --- |
| **BIRCOtop attachment elements 40 x 40**+ Circumferential perforation+ Length 250 mm + Width 250 mm+ Construction height adjustable on-site 59 to 170 mmmade of galvanized steel[ ] \_\_\_\_\_ pce BIRCOtop attachment element 40 x 40  construction height 59-83 / 82-117 / 115-170,  load class walkabledelivery and installation according to manufacturer’s installation instructions.Manufacturer: BIRCO GmbHHerrenpfädel 142, D 76532 Baden-BadenPhone +497221 - 5003-0; Fax +497221 - 5003-1149; www.birco.de | **Unit price** | **Total price** |
| **BIRCOtop accessories 40 x 40 – Gratings**+ Width 392 mm+ Length 392 mm+ Height 20 mmwith 1-point M10/A2 bolt connection[ ] \_\_\_\_\_ pce punched hole grating – circular holes, made of hot- dipped galvanized steel, load class walkable[ ] \_\_\_\_\_ pce slot grating made of hot-dipped galvanized steel,  load class walkable [ ] \_\_\_\_\_ pce mesh grating made of hot-dipped galvanized steel,  mesh width 30/10, load class walkabledelivery and installation according to manufacturer’s installation instructions.Manufacturer:BIRCO GmbH | **Unit price** | **Total price** |
| **BIRCOtop – Branch channel**+ Perforated on both sides+ Width 100 mm, length 2000 mm+ Height 30 mm[ ] \_\_\_\_\_ pce branch channel made of hot-dipped galvanized  steel, load class walkabledelivery and installation according to manufacturer’s installation instructions.Manufacturer:BIRCO GmbH | **Unit price** | **Total price** |