|  |  |  |
| --- | --- | --- |
| **BIRCOtopline 130 – Drainage channel without visible edge**  + Perforated on one side  + Simple installation from above with plug-in system  + With screw thread for leveling feet  + Length 500 / 1000 / 3000 mm  + Width at top 130 mm, at ground 99 mm  + Construction height 50 / 75 mm  made of galvanized steel  [ ] \_\_\_\_\_ pce BIRCOtopline 130, channel construction height   50/75, load class walkable, length 500/1000/3000   mm  delivery and installation according to manufacturer’s installation instructions.  Manufacturer:  BIRCO GmbH Herrenpfädel 142, D 76532 Baden-Baden Phone +497221 - 5003-0; Fax +497221 - 5003-1149; www.birco.de | **Unit price** | **Total price** |
| **BIRCOtopline 130 – corner piece 90 ° without visible edge**  + Perforated on one side  + Simple installation from above with plug-in system  + With screw thread for leveling feet  + Length 500 x 500 mm  + Width at top 130 mm, at ground 99 mm  + Construction height 50 / 75 mm  made of galvanized steel  [ ] \_\_\_\_\_ pce BIRCOtopline 130, corner piece 90°, construction   height 50/75, load class walkable, perforation inside /   outside  delivery and installation according to manufacturer’s installation instructions.  Manufacturer:  BIRCO GmbH | **Unit price** | **Total price** |
| **BIRCOtopline 130 – End caps**  + Width 130 mm  + For construction height 50 / 75 mm  made of galvanized steel  [ ] \_\_\_\_\_ pce BIRCOtopline 130 end cap for construction height   50 / 75  delivery and installation according to manufacturers installation instructions.  Manufacturer:  BIRCO GmbH | **Unit price** | **Total price** |

|  |  |  |
| --- | --- | --- |
| **BIRCOtopline 130 – Gratings with clamping device**  + Width 122 mm  + Height 20 mm  + Load class: walkable  [ ] \_\_\_\_\_ pce punched hole grating – circular holes Ø 8 mm,  made of galvanized steel, length 500 / 1000 mm  [ ] \_\_\_\_\_ pce punched hole grating – square holes 8 x 8 mm, made of galvanized steel, length 500 / 1000 mm  [ ] \_\_\_\_\_ pce slot grating made of galvanized steel,   length 500 / 1000 mm  [ ] \_\_\_\_\_ pce mesh grating made of galvanized steel,   length 500 / 1000 mm, mesh width 30/10  delivery and installation according to manufacturers installation instructions.  Manufacturer:  BIRCO GmbH | **Unit price** | **Total price** |
| **BIRCOtopline 130 – Gratings with clamping device for corner piece 90°**  + Width 122 mm  + Height 20 mm  + Load class: walkable  [ ] \_\_\_\_\_ pce punched hole grating – circular holes Ø 8 mm,  made of galvanized steel, length 500 x 500 mm  [ ] \_\_\_\_\_ pce punched hole grating – square holes 8 x 8 mm, made of galvanized steel, length 500 x 500 mm  [ ] \_\_\_\_\_ pce slot grating made of galvanized steel,   length 500 x 500 mm  [ ] \_\_\_\_\_ pce mesh grating made of galvanized steel,   length 500 x 500 mm, mesh width 30/10  delivery and installation according to manufacturers installation instructions.  Manufacturer:  BIRCO GmbH | **Unit price** | **Total price** |
| **BIRCOtopline 130 – Set of leveling feet**  + Galvanized steel  + Set of 4 continuously adjustable leveling feet  + Load class: walkable  [ ] \_\_\_\_\_ BIRCOtopline 130 set of 4 leveling feet  delivery and installation according to manufacturers installation instructions.  Manufacturer:  BIRCO GmbH | **Unit price** | **Total price** |

|  |  |  |
| --- | --- | --- |
| **BIRCOtopline 130 – Gravel strip**  + Galvanized steel  + For construction height 50 and 75 mm  + Width 35 x 45 mm  [ ] \_\_\_\_\_ BIRCOtopline 130 gravel strip, length 500 / 1000 mm  delivery and installation according to manufacturers installation instructions.  Manufacturer:  BIRCO GmbH | **Unit price** | **Total price** |