|  |  |  |
| --- | --- | --- |
| **BIRCOdicht NW 150 - 300 – In-line outfall unit with shut-off valve**for 1- or 2-sided channel connection, including stainless steel L angle frame (V2A - also removable)+ Manually operated valve flap DN 150+ On request also with pneumatical valve flap+ PEHD lining+ Drain direction in accordance with the customer’s wishes+ PEHD-pipe socket DA 160 – SDR 17, 300 mm long+ Length 500 mm+ Width 470 mmmade of concrete C 40/50 according to EN 1433, up to load class F 900 as defined by EN 1433, with visible sealing joint[ ] \_\_\_\_\_ pce in-line outfall unit(s) 1 piece, construction height  with angles 805 mmdelivery and installation according to manufacturer’s installation instructions.Manufacturer:BIRCO GmbHHerrenpfädel 142, D 76532 Baden-BadenPhone +497221 - 5003-0; Fax +497221 - 5003-1149; www.birco.de | **Unit price** | **Total price** |
| **BIRCOdicht NW 150 - 300 – Gratings for in-line outfall unit with shut-off valve**+ Width 437 mm+ Height 45 mm+ With keybushingload class according to DIN EN 1433, with 4 point per grating M12/A2-bolt fastening[ ] \_\_\_\_\_ pce cast twofold slotted gratings black immersion- lacquered, length 500 mm, load class F 900delivery and installation according to manufacturer’s installation instructions.Manufacturer: BIRCO GmbH | **Unit price** | **Total price** |
| **BIRCOsolid NW 150 - 300 – Service key**+ For in-line outfall unit with shut-off valve+ For manuel operation[ ] \_\_\_\_\_ pce service keydelivery.Manufacturer:BIRCO GmbH | **Unit price** | **Total price** |