|  |  |  |
| --- | --- | --- |
| **BIRCOdicht NW 200 - Drainage channel with 0.5 % inbuilt fall**  + PEHD lining  + Length 2000 mm  + Width 350 mm  + Construction height at groove/tongue 315 to 415 mm including   edge angle  + With German Technical Approval (certificate no. Z-74.4-52)  made of concrete C 40/50 according to EN 1433, up to load class F 900 as defined by EN 1433, structural variations in accordance with customer wishes, with visible sealing joint  [ ] \_\_\_\_\_ m BIRCOdicht NW 200 channel no. 1/2 – 19/20  including the necessary end caps, delivery and installation according to manufacturer’s installation instructions.  Manufacturer: BIRCO GmbH Herrenpfädel 142, D 76532 Baden-Baden Phone +497221 - 5003-0; Fax +497221 - 5003-1149; www.birco.de | **Unit price** | **Total price** |
| **BIRCOdicht NW 200 – Drainage channel without inbuilt fall**  + PEHD lining  + Length 2000 mm  + Width 350 mm  + Construction height at groove/tongue 315/365/415 mm   including edge angle  + With German Technical Approval (certificate no. Z-74.4-52)  made of concrete C 40/50 according to EN 1433, up to load class F 900 as defined by EN 1433, structural variations in accordance with customer wishes, with visible sealing joint  [ ] \_\_\_\_\_ m BIRCOdicht NW 200 channel no. 0/0 / 10/0 / 20/0  including the necessary end caps, delivery and installation according to manufacturer’s installation instructions.  Manufacturer: BIRCO GmbH | **Unit price** | **Total price** |

|  |  |  |
| --- | --- | --- |
| **BIRCOdicht NW 200 – Corner piece 90°**  + PEHD lining  + Length 835 mm  + Width 515 mm  + Construction height 315/365/415 mm including edge angle  + With German Technical Approval (certificate no. Z-74.4-52)  made of concrete C 40/50 according to EN 1433, up to load class F 900 as defined by EN 1433, structural variations in accordance with customer wishes, with visible sealing joint  [ ] \_\_\_\_\_ pce corner piece(s) no. 0/0 / 10/0 / 20/0  including the necessary end caps, delivery and installation according to manufacturer’s installation instructions.  Manufacturer: BIRCO GmbH | **Unit price** | **Total price** |
| **BIRCOdicht NW 200 – T-piece 90°**  + PEHD lining  + Length 1500 mm  + Width 850 mm  + Construction height with angle 315/365/415 mm  + With German Technical Approval (certificate no. Z-74.4-52)  made of concrete C 40/50 according to EN 1433, up to load class F 900 as defined by EN 1433, structural variations in accordance with customer wishes, with visible sealing joint  [ ] \_\_\_\_\_ pce T-piece(s) no. 0/0 / 10/0 / 20/0  including the necessary end caps, delivery and installation according to manufacturer’s installation instructions.  Manufacturer: BIRCO GmbH | **Unit price** | **Total price** |
| **BIRCOdicht NW 200 – L-angles removable**  + Thickness 4 mm  + Length 980 mm  + Width 64 mm  + Height 39 mm  [ ] \_\_\_\_\_ pce L-angles galvanized  [ ] \_\_\_\_\_ pce L-angles stainless steel  Assembled ex-factory, delivery.  Manufacturer: BIRCO GmbH | **Unit price** | **Total price** |

|  |  |  |
| --- | --- | --- |
| **BIRCOdicht NW 200 – End caps and outlet sockets**  + Width 350 mm  + Drain length 300 mm  [ ] \_\_\_\_\_ pce end cap(s) PEHD, no. 0/0 – 10 / 11 - 20  [ ] \_\_\_\_\_ pce end caps(s) with outlet DA 225-SDR 17 PEHD   no. 0/0 - 10 / 11 – 20/0  [ ] \_\_\_\_\_ pce outlet socket(s) DA 160–SDR17  Assembled ex-factory, delivery.  Manufacturer: BIRCO GmbH | **Unit price** | **Total price** |
| **BIRCOdicht NW 200 – In-line outfall unit** for 1- or 2-sided channel connection  + PEHD lining  + PEHD-pipe socket DA 225 – SDR 17, 300 mm long  + Length 500 mm  + Width 350mm  + With German Technical Approval (certificate no. Z-74.4-52)  made of concrete C 40/50 according to EN 1433, up to load class F 900 as defined by EN 1433, structural variations in accordance with customer wishes, with visible sealing joint  [ ] \_\_\_\_\_ pce in-line outfall unit(s) 1 piece, construction height   with angles 805 mm  including the necessary end caps, delivery and installation according to manufacturer’s installation instructions.  Manufacturer: BIRCO GmbH | **Unit price** | **Total price** |
| **BIRCOdicht NW 200 – Gratings**  + Width 317 mm  + Height 35 mm  load class according to DIN EN 1433, with 8 point per metre M12/A2-bolt fastening, mesh grating 4 point fastening per grating  [ ] \_\_\_\_\_ pce cast slotted gratings black immersion-lacquered, length 500 mm, load class F 900  [ ] \_\_\_\_\_ pce mesh grating black immersion-lacquered, length 500 mm, load class E 600  delivery and installation according to manufacturer’s installation instructions.  Manufacturer: BIRCO GmbH | **Unit price** | **Total price** |