|  |  |  |
| --- | --- | --- |
| **BIRCOdicht NW 300 – Drainage channel with 0.5 % inbuilt fall** + PEHD lining+ Length 2000 mm+ Width 470 mm+ Construction height at groove/tongue 475 to 575 mm including edge angle+ With German Technical Approval (certificate no. Z-74.4-52)made of concrete C 40/50 according to EN 1433, up to load class F 900 as defined by EN 1433, structural variations in accordance with customer wishes, with visible sealing joint[ ] \_\_\_\_\_ m BIRCOdicht NW 300 channel no. 1/2 – 19/20including the necessary end caps, delivery and installation according to manufacturer’s installation instructions.Manufacturer: BIRCO GmbHHerrenpfädel 142, D 76532 Baden-BadenPhone +497221 - 5003-0; Fax +497221 - 5003-1149; www.birco.de | **Unit price** | **Total price** |
| **BIRCOdicht NW 300 – Drainage channel without inbuilt fall**+ PEHD lining+ Length 2000 mm+ Width 470 mm+ Construction height at groove/tongue 475/525/575 mm including edge angle+ With German Technical Approval (certificate no. Z-74.4-52)made of concrete C 40/50 according to EN 1433, up to load class F 900 as defined by EN 1433, structural variations in accordance with customer wishes, with visible sealing joint [ ] \_\_\_\_\_ m BIRCOdicht NW 300 channel no. 0/0 / 10/0 / 20/0including the necessary end caps, delivery and installation according to manufacturer’s installation instructions.Manufacturer:BIRCO GmbH | **Unit price** | **Total price** |

|  |  |  |
| --- | --- | --- |
| **BIRCOdicht NW 300 – Corner piece 90°**+ PEHD lining+ Length 955 mm+ Width 515 mm+ Construction height 475/525/575 mm including edge angle+ With German Technical Approval (certificate no. Z-74.4-52)made of concrete C 40/50 according to EN 1433, up to load class F 900 as defined by EN 1433, structural variations in accordance with customer wishes, with visible sealing joint[ ] \_\_\_\_\_ pce corner piece(s) no. 0/0 / 10/0 / 20/0including the necessary end caps, delivery and installation according to manufacturer’s installation instructions.Manufacturer:BIRCO GmbH | **Unit price** | **Total price** |
| **BIRCOdicht NW 300 – T-piece 90°**+ PEHD lining+ Length 1500 mm+ Width 970 mm+ Construction height with angle 475/525/575 mm+ With German Technical Approval (certificate no. Z-74.4-52)made of concrete C 40/50 according to EN 1433, up to load class F 900 as defined by EN 1433, structural variations in accordance with customer wishes, with visible sealing joint[ ] \_\_\_\_\_ pce T-piece(s) no. 0/0 / 10/0 / 20/0including the necessary end caps, delivery and installation according to manufacturer’s installation instructions.Manufacturer:BIRCO GmbH | **Unit price** | **Total price** |
| **BIRCOdicht NW 300 – L-angles removable**+ Thickness 4 mm+ Length 980 mm+ Width 73 mm+ Height 49 mm[ ] \_\_\_\_\_ pce L-angles galvanized[ ] \_\_\_\_\_ pce L-angles stainless steelAssembled ex-factory, delivery.Manufacturer:BIRCO GmbH | **Unit price** | **Total price** |

|  |  |  |
| --- | --- | --- |
| **BIRCOdicht NW 300 – End caps and outlet sockets**+ Width 470 mm+ Drain length 300 mm[ ] \_\_\_\_\_ pce end cap(s) PEHD, no. 0/0 – 10 / 11 - 20[ ] \_\_\_\_\_ pce end caps(s) with outlet DA 315-SDR 17 PEHD  no. 0/0 - 10 / 11 – 20/0[ ] \_\_\_\_\_ pce outlet socket(s) DA 315–SDR17Assembled ex-factory, delivery.Manufacturer:BIRCO GmbH | **Unit price** | **Total price** |
| **BIRCOdicht NW 300 – In-line outfall unit** for 1- or 2-sided channel connection+ PEHD lining+ PEHD-pipe socket DA 315 – SDR 17, 300 mm long+ Length 500 mm+ Width 470mm+ With German Technical Approval (certificate no. Z-74.4-52)made of concrete C 40/50 according to EN 1433, up to load class F 900 as defined by EN 1433, structural variations in accordance with customer wishes, with visible sealing joint[ ] \_\_\_\_\_ pce in-line outfall unit(s) 1 piece, construction height  with angles 805 mmdelivery and installation according to manufacturer’s installation instructions.Manufacturer:BIRCO GmbH | **Unit price** | **Total price** |
| **BIRCOdicht NW 300 – Gratings**+ Width 437 mm+ Height 45 mmload class according to DIN EN 1433, with 8 point per metre M12/A2-bolt fastening[ ] \_\_\_\_\_ pce cast twofold slotted gratings black immersion- lacquered, length 500 mm, load class F 900delivery and installation according to manufacturer’s installation instructions.Manufacturer:BIRCO GmbH | **Unit price** | **Total price** |