|  |  |  |
| --- | --- | --- |
| **BIRCOdicht Point drainage - Base shut-off outfall unit as point feed inlet** without channel connection  + Manually operated valve flap DN 150 (Also available with   pneumatical valve flap)  + PEHD lining  + Including stainless steel L angle frame (V2A - also removable)  + PEHD-pipe socket DA 160 – SDR 17, 300 mm long  + Drain direction in accordance with the customer’s wishes  + Length 500 mm  + Width 470mm  made of concrete C 40/50 according to EN 1433, up to load class E 600 as defined by EN 1433, with visible sealing joint  [ ] \_\_\_\_\_ pce bas shut off outfall unit, 1 piece, construction   height with angles 805 mm  delivery and installation according to manufacturer’s installation instructions.  Manufacturer:  BIRCO GmbH Herrenpfädel 142, D 76532 Baden-Baden Phone +497221 - 5003-0; Fax +497221 - 5003-1149; www.birco.de | **Unit price** | **Total price** |
| **BIRCOdicht Point drainage – Gratings for base shut-off outfall unit**  + With keybushing  + Width 437 mm  + Height 45 mm  load class according to DIN EN 1433, with 4 point per grating M12/A2-bolt fastening  [ ] \_\_\_\_\_ pce cast slotted gratings, two-fold, black immersion-  lacquered, length 500 mm, load class E 600  delivery and installation according to manufacturer’s installation instructions.  Manufacturer: BIRCO GmbH | **Unit price** | **Total price** |

|  |  |  |
| --- | --- | --- |
| **BIRCOdicht Point drainage –outfall unit 40/40** without channel connection  + Stainless steel frame (V2A, removable)  + PEHD lining  + PEHD-pipe socket DA 225 – SDR 17, 300 mm long  + Length 400 mm  + Width 400mm  made of concrete C 40/50 according to EN 1433, up to load class F 900 as defined by EN 1433  [ ] \_\_\_\_\_ pce outfall unit, 1-teilig, 1 piece, construction height   1250 mm  delivery and installation according to manufacturer’s installation instructions.  Manufacturer: BIRCO GmbH Herrenpfädel 142, D 76532 Baden-Baden Tel. 07221 - 5003-0; Fax 07221 - 5003-47; www.birco.de | **Unit price** | **Total price** |
| **BIRCOdicht Point drainage – Gratings for outfall unit 40/40**  + Width 380 mm  + Height 40 mm  load class according to DIN EN 1433, with 4 point per grating M12/A2-bolt fastening  [ ] \_\_\_\_\_ pce cast slotted gratings, two-fold, black immersion-  lacquered, length 380 mm, load class E 600  [ ] \_\_\_\_\_ pce mesh gratings galvanized steel,   mesh width 20-30 / 20-12 mm  length 380 mm, load class E 600  delivery and installation according to manufacturer’s installation instructions.  Manufacturer: BIRCO GmbH | **Unit price** | **Total price** |
| **BIRCOdicht Point drainage - Sump well**  + Stainless steel frame (V2A)  + PEHD lining  + Length 950 mm  + Width 950mm  made of concrete C 40/50 according to EN 1433, up to load class E 600 as defined by EN 1433  [ ] \_\_\_\_\_ pce sump well, 1-teilig, construction height   with angles900 mm  delivery and installation according to manufacturer’s installation instructions.  Manufacturer: BIRCO GmbH Herrenpfädel 142, 76532 Baden-Baden Tel. 07221 - 5003-0; Fax 07221 - 5003-47; www.birco.de | **Unit price** | **Total price** |
| **BIRCOdicht Point drainage – Gratings for sump well**  + 2-piece  + Width 916 mm  + Height 35 mm  load class according to DIN EN 1433, with 4 point per grating M12/A2-bolt fastening  [ ] \_\_\_\_\_ pce mesh gratings galvanized steel   length 916 mm, load class C 250  delivery and installation according to manufacturer’s installation instructions.  Manufacturer: BIRCO GmbH | **Unit price** | **Total price** |