|  |  |  |
| --- | --- | --- |
| **BIRCOdicht Point drainage - Base shut-off outfall unit as point feed inlet** without channel connection+ Manually operated valve flap DN 150 (Also available with  pneumatical valve flap)+ PEHD lining+ Including stainless steel L angle frame (V2A - also removable)+ PEHD-pipe socket DA 160 – SDR 17, 300 mm long+ Drain direction in accordance with the customer’s wishes+ Length 500 mm+ Width 470mmmade of concrete C 40/50 according to EN 1433, up to load class E 600 as defined by EN 1433, with visible sealing joint[ ] \_\_\_\_\_ pce bas shut off outfall unit, 1 piece, construction  height with angles 805 mmdelivery and installation according to manufacturer’s installation instructions.Manufacturer: BIRCO GmbHHerrenpfädel 142, D 76532 Baden-BadenPhone +497221 - 5003-0; Fax +497221 - 5003-1149; www.birco.de | **Unit price** | **Total price** |
| **BIRCOdicht Point drainage – Gratings for base shut-off outfall unit**+ With keybushing+ Width 437 mm+ Height 45 mmload class according to DIN EN 1433, with 4 point per grating M12/A2-bolt fastening[ ] \_\_\_\_\_ pce cast slotted gratings, two-fold, black immersion- lacquered, length 500 mm, load class E 600delivery and installation according to manufacturer’s installation instructions.Manufacturer:BIRCO GmbH | **Unit price** | **Total price** |

|  |  |  |
| --- | --- | --- |
| **BIRCOdicht Point drainage –outfall unit 40/40** without channel connection+ Stainless steel frame (V2A, removable)+ PEHD lining+ PEHD-pipe socket DA 225 – SDR 17, 300 mm long+ Length 400 mm+ Width 400mmmade of concrete C 40/50 according to EN 1433, up to load class F 900 as defined by EN 1433 [ ] \_\_\_\_\_ pce outfall unit, 1-teilig, 1 piece, construction height  1250 mmdelivery and installation according to manufacturer’s installation instructions.Manufacturer:BIRCO GmbHHerrenpfädel 142, D 76532 Baden-BadenTel. 07221 - 5003-0; Fax 07221 - 5003-47; www.birco.de | **Unit price** | **Total price** |
| **BIRCOdicht Point drainage – Gratings for outfall unit 40/40**+ Width 380 mm+ Height 40 mmload class according to DIN EN 1433, with 4 point per grating M12/A2-bolt fastening[ ] \_\_\_\_\_ pce cast slotted gratings, two-fold, black immersion- lacquered, length 380 mm, load class E 600[ ] \_\_\_\_\_ pce mesh gratings galvanized steel,  mesh width 20-30 / 20-12 mm length 380 mm, load class E 600delivery and installation according to manufacturer’s installation instructions.Manufacturer:BIRCO GmbH | **Unit price** | **Total price** |
| **BIRCOdicht Point drainage - Sump well**+ Stainless steel frame (V2A)+ PEHD lining+ Length 950 mm+ Width 950mmmade of concrete C 40/50 according to EN 1433, up to load class E 600 as defined by EN 1433[ ] \_\_\_\_\_ pce sump well, 1-teilig, construction height  with angles900 mmdelivery and installation according to manufacturer’s installation instructions.Manufacturer:BIRCO GmbHHerrenpfädel 142, 76532 Baden-BadenTel. 07221 - 5003-0; Fax 07221 - 5003-47; www.birco.de | **Unit price** | **Total price** |
| **BIRCOdicht Point drainage – Gratings for sump well**+ 2-piece+ Width 916 mm+ Height 35 mmload class according to DIN EN 1433, with 4 point per grating M12/A2-bolt fastening[ ] \_\_\_\_\_ pce mesh gratings galvanized steel  length 916 mm, load class C 250delivery and installation according to manufacturer’s installation instructions.Manufacturer:BIRCO GmbH | **Unit price** | **Total price** |