|  |  |  |
| --- | --- | --- |
| **BIRCOprotect NW 200 – Drainage channel with 0.5 % inbuilt fall with German Technical approval**  + Length 1000 mm  + Width at top 330 mm, width at bottom 335 mm  + Construction height at groove/tongue 310 to 360 mm  + With German Technical Approval (certificate no. Z-74.4-34)  made of concrete C 40/50 according to EN 1433, up to load class F 900 as defined by EN 1433, with anchored 4 mm hot-dipped galvanized solid steel angles for combi-closure system (70 µm zinc coating), with visible sealing joint  [ ] \_\_\_\_\_ m BIRCOprotect NW 200 channel no. 1 - 10  including necessary end caps, delivery and installation according to manufacturer’s installation instructions.  Manufacturer:  BIRCO GmbH Herrenpfädel 142, D 76532 Baden-Baden Phone +497221 - 5003-0; Fax +497221 - 5003-1149; www.birco.de | **Unit price** | **Total price** |
| **BIRCOprotect NW 200 – Drainage channel without inbuilt fall with German Technical Approval**  + Length 500 mm (only for height 310 mm)/1000 mm  + Width at top 330 mm, width at bottom 335 mm  + Construction height 310/335/360 mm  + With German Technical Approval (certificate no. Z-74.4-34)  made of concrete C 40/50 according to EN 1433, up to load class F 900 as defined by EN 1433, with anchored 4 mm hot-dipped galvanized solid steel angles for combi-closure system (70 µm zinc coating), with visible safety sealing joint  [ ] \_\_\_\_\_ m BIRCOprotect NW 200 channel  including necessary end caps, delivery and installation according to manufacturer’s installation instructions.  Manufacturer: BIRCO GmbH | **Unit price** | **Total price** |
| **BIRCOprotect NW 200 – End caps and end caps with outlet DN 200**  + Width 330 mm  Made of galvanized steel  [ ] \_\_\_\_\_ pce of end cap for channel no. 0/0–6 / 7–10  [ ] \_\_\_\_\_ pce of end cap with outlet DN 200 for channel no. 0/0   / 5/0 / 10/0  [ ] \_\_\_\_\_ pce of end cap with outlet DA 200 x 4,9 – SDR 41,   PEHD for channel no. 0/0 / 5/0 / 10/0, length 300 mm delivery.  Manufacturer: BIRCO GmbH | **Unit price** | **Total price** |

|  |  |  |
| --- | --- | --- |
| **BIRCOprotect NW 200 – In-line outfall unit**  **with PEHD pipe connector** for 1- or 2-sided channel connection  + Galvanized silt bucket  + PEHD pipe connector DA 200 x 4,9 – SDR 41, length 300 mm  + Length at top 500 mm, length at bottom 510 mm  + Width at top 330 mm, width at bottom 345mm  made of concrete C 40/50 according to EN 1433, up to load class F 900 as defined by EN 1433, with anchored 4 mm hot-dipped galvanized solid steel angles for combi-closure system (70 µm zinc coating), with visible safety sealing joint  [ ] \_\_\_\_\_ pce of in-line outfall unit(s), 1 piece, construction   height 725 mm,  including necessary end caps, delivery and installation according to manufacturer’s installation instructions.  Manufacturer: BIRCO GmbH | **Unit price** | **Total price** |
| **BIRCOprotect NW 200 – Gratings**  + Width 317 mm  + Width 35 mm  load class according to DIN EN 1433, with 8-point per metre M12/A2-bolt fastening  [ ] \_\_\_\_\_ pce cast slotted grating black immersion-lacquered, length 500 mm, load class F 900  delivery and installation according to manufacturer’s installation instructions.  Manufacturer: BIRCO GmbH | **Unit price** | **Total price** |
| **BIRCOprotect NW 200 – Cutting of channels including grating** and painting or galvanizing of cut angles and gratings.  [ ] \_\_\_\_\_ 90° cut  [ ] \_\_\_\_\_ Mitre cut according to degree specification  Manufacturer: BIRCO GmbH | **Unit price** | **Total price** |
| **BIRCOprotect NW 200 – Hole drilling of channel**  [ ] \_\_\_\_\_ in horizontal / vertical direction, diameter DN 200  [ ] \_\_\_\_\_ pce of silt bucket(s)  Delivery.  Manufacturer: BIRCO GmbH | **Unit price** | **Total price** |