|  |  |  |
| --- | --- | --- |
| **BIRCOprotect NW 300 – Drainage channel without inbuilt fall with German Technical Approval**+ Length 1000 mm / 2000 mm+ Width at top 450 mm, width at bottom 460 mm+ Construction height 470 mm+ mit bauaufsichtlicher Zulassung Nr. Z-74.4-34+ With German Technical Approval (certificate no. Z-74.4-34)made of concrete C 40/50 according to EN 1433, up to load class F 900 as defined by EN 1433, with anchored 4 mm hot-dipped galvanized solid steel angles for combi-closure system (70 µm zinc coating), with visible safety sealing joint[ ] \_\_\_\_\_ m BIRCOprotect NW 300 channel including necessary end caps, delivery and installation according to manufacturer’s installation instructions.Manufacturer: BIRCO GmbHHerrenpfädel 142, D 76532 Baden-BadenPhone +497221 - 5003-0; Fax +497221 - 5003-1149; www.birco.de | **Unit price** | **Total price** |
| **BIRCOprotect NW 300 – End caps and end caps with outlet DN 200**+ Width 450 mmMade of galvanized steel[ ] \_\_\_\_\_ pce of end cap for channel no. 0/0 [ ] \_\_\_\_\_ pce of end cap with outlet DN 200 for channel no. 0/0[ ] \_\_\_\_\_ pce of end cap with outlet DA 315 x 17,9 –  SDR 17, PEHD for channel no. 0/0, length 300 mmdelivery.Manufacturer:BIRCO GmbH | **Unit price** | **Total price** |
| **BIRCOprotect NW 300 – In-line outfall unit with cast-in pipe connector** for 1- or 2-sided channel connection+ Galvanized silt bucket+ Cast-in pipe connector for DN 300 pipe+ Length 500 mm+ Width at top 450 mm, width at bottom 510mm,made of concrete C 40/50 according to EN 1433, up to load class F 900 as defined by EN 1433, with anchored 4 mm hot-dipped galvanized solid steel angles for combi-closure system (70 µm zinc coating), with visible safety sealing joint[ ] \_\_\_\_\_ pce of in-line outfall unit(s), 1 piece, construction  height 980 mmincluding necessary end caps, delivery and installation according to manufacturer’s installation instructions.Manufacturer:BIRCO GmbH | **Unit price** | **Total price** |

|  |  |  |
| --- | --- | --- |
| **BIRCOprotect NW 300 – In-line outfall unit with PEHD pipe connector** for 1- or 2-sided channel connection+ Galvaniued silt bucket+ PEHD pipe connector DA 315 x 17,9 – SDR 17, length 300 mm+ Length 500 mm+ Width at top 450 mm, width at bottom 510 mmmade of concrete C 40/50 according to EN 1433, up to load class F 900 as defined by EN 1433, with anchored 4 mm hot-dipped galvanized solid steel angles for combi-closure system (70 µm zinc coating), with visible safety sealing joint[ ] \_\_\_\_\_ pce of in-line outfall unit(s), 1 piece, construction  height 980 mmincluding necessary end caps, delivery and installation according to manufacturer’s installation instructions.Manufacturer:BIRCO GmbH | **Unit price** | **Total price** |
| **BIRCOprotect NW 300 – Grating**+ Width 437 mm+ Height 45 mmload class according to DIN EN 1433, with 8-point per metre M16/A2-bolt fastening[ ] \_\_\_\_\_ pce cast twofold slotted grating black immersion- lacquered, length 500 mm, load class F 900delivery and installation according to manufacturer’s installation instructions.Manufacturer:BIRCO GmbH | **Unit price** | **Total price** |
| **BIRCOprotect NW 300 – Shut-off outfall unit NW 300 for channel NW 100 to 300**for 1- or 2-sided channel connection up to NW 300 + Manually / electrical / pneumatical operated valve flap DN 150+ Galvanized silt bucket+ PEHD pipe connector DA 160 x 9,1 – SDR 17, length 300 mm+ Pipe connector at right angles to channel line+ Not covered by German Technical Approval certificate+ Length 500 mm+ Width at top 450 mm, width at bottom 510 mmmade of concrete C 40/50 according to EN 1433, up to load class F 900 as defined by EN 1433, with anchored 4 mm hot-dipped galvanized solid steel angles for combi-closure system (70 µm zinc coating), with visible safety sealing joint[ ] \_\_\_\_\_ pce shut-off outfall unit, 1-piece, construction height  980 mmincluding necessary end caps, delivery and installation according to manufacturer’s installation instructions.Manufacturer:BIRCO GmbH | **Unit price** | **Total price** |
| **BIRCOprotect NW 300 – Gratings for shut-off outfall unit**+ Width 437 mm+ Height 45 mm+ mit Schlüsseldurchführung+ With key bushingload class according to DIN EN 1433, with 4-point per grating M16/A2-bolt fastening[ ] \_\_\_\_\_ pce cast twofold slotted grating black immersion- lacquered, length 500 mm, load class E 600delivery and installation according to manufacturer’s installation instructions Manufacturer:BIRCO GmbH | **Unit price** | **Total price** |
| **BIRCOprotect NW 300 – utting of channel including grating** and painting or galvanizing of cut angles and gratings.[ ] \_\_\_\_\_ 90° cut[ ] \_\_\_\_\_ Mitre cut according to degree specificationManufacturer:BIRCO GmbH | **Unit price** | **Total price** |
| **BIRCOprotect NW 300 – Hole drilling of channel**[ ] \_\_\_\_\_ in horizontal / vertical direction, diameter DN 300[ ] \_\_\_\_\_ pce of silt bucket(s)Delivery.Manufacturer: BIRCO GmbH | **Unit price** | **Total price** |
| **BIRCOprotect NW 300 – Service key**+ For shut-off outfall unit+ For manual operation[ ] \_\_\_\_\_ pce service keyManufacturer:BIRCO GmbH | **Unit price** | **Total price** |