|  |  |  |
| --- | --- | --- |
| **Sealant**[ ] BIRCO Primer K1 for non-absorbent surfaces such as glass,  enamel, stainless steel, galvanised steel, ceramic tiles, etc.[ ] BIRCO Primer K2 for absorbent surfaces such as concrete,  aerated concrete, stone, plaster, etc.[ ] PE cord[ ] BIRCOplast two-part, permanently elastic  polysulfide-based sealant that is resistant to mineral  oil and fuelsSealing according to manufacturer’s installation instructions.Manufacturer: BIRCO GmbHHerrenpfädel 142, D 76532 Baden-BadenPhone +497221 - 5003-0; Fax +497221 - 5003-1149; www.birco.de | **Unit price** | **Total price** |
| **Tools**[ ] Tool cleaner[ ] Cartridge base[ ] Cartridge gun[ ] Mixer blade[ ] Tool set includes a cartridge gun with 3 nozzles, hand  mixer (stand pipe and foot), mixer blade Delivery.Manufacturer: BIRCO GmbH | **Unit price** | **Total price** |