|  |  |  |
| --- | --- | --- |
| **Sealant**  [ ] BIRCO Primer K1 for non-absorbent surfaces such as glass,   enamel, stainless steel, galvanised steel, ceramic tiles, etc.  [ ] BIRCO Primer K2 for absorbent surfaces such as concrete,   aerated concrete, stone, plaster, etc.  [ ] PE cord  [ ] BIRCOplast two-part, permanently elastic   polysulfide-based sealant that is resistant to mineral   oil and fuels  Sealing according to manufacturer’s installation instructions.  Manufacturer:  BIRCO GmbH Herrenpfädel 142, D 76532 Baden-Baden Phone +497221 - 5003-0; Fax +497221 - 5003-1149; www.birco.de | **Unit price** | **Total price** |
| **Tools**  [ ] Tool cleaner  [ ] Cartridge base  [ ] Cartridge gun  [ ] Mixer blade  [ ] Tool set includes a cartridge gun with 3 nozzles, hand   mixer (stand pipe and foot), mixer blade  Delivery.  Manufacturer:  BIRCO GmbH | **Unit price** | **Total price** |