|  |  |  |
| --- | --- | --- |
| **BIRCOcanal NW 1000 – Supply channels without angles**  + Length 2000 mm  + External width 1200 mm, internal width 1000 mm  + External construction height 600 mm, internal height 500 mm  + Cast-in anchor sleeves RD 14 per cover for mechanical installation  made of reinforced grade concrete C 40/50, CE compliance with EN 1433, up to load class E 600 as defined by EN 1433, with safety sealing joint  [ ] \_\_\_\_\_ m BIRCOcanal NW 1000 channel   with cast-in mounting rails  [ ] \_\_\_\_\_ m BIRCOcanal NW 1000 channel without mounting rails  [ ] Sealing with SF-Connect  delivery and installation according to manufacturer’s installation instructions.  Manufacturer:  BIRCO GmbH Herrenpfädel 142, D 76532 Baden-Baden Phone +497221 - 5003-0; Fax +497221 - 5003-1219; www.birco.de | **Unit price** | **Total price** |
| **BIRCOcanal NW 1000 – Covers**  + Width 1200 mm  + Height 165 mm  + 2 cast-in anchor sleeves RD 14 per cover for mechanical   installation  [ ] \_\_\_\_\_ pce reinforced concrete cover with smooth surface   length 2000 mm, load class SLW 60  delivery and installation according to manufacturer’s installation instructions.  Manufacturer: BIRCO GmbH | **Unit price** | **Total price** |
| **BIRCOcanal NW 1000 – Cutting of channels including cover**  [ ] \_\_\_\_\_ Channel section 90°  [ ] \_\_\_\_\_ Mitre cut according to degree specification  Manufacturer: BIRCO GmbH | **Unit price** | **Total price** |
| **BIRCOcanal NW 1000 – Drilled hole in channel base**  [ ] \_\_\_\_\_ in horizontal / vertical direction, diameter DN 300  Delivery.  Manufacturer: BIRCO GmbH | **Unit price** | **Total price** |