|  |  |  |
| --- | --- | --- |
| **BIRCOcanal NW 1000 – Supply channels without angles**+ Length 2000 mm+ External width 1200 mm, internal width 1000 mm+ External construction height 600 mm, internal height 500 mm+ Cast-in anchor sleeves RD 14 per cover for mechanical installationmade of reinforced grade concrete C 40/50, CE compliance with EN 1433, up to load class E 600 as defined by EN 1433, with safety sealing joint[ ] \_\_\_\_\_ m BIRCOcanal NW 1000 channel  with cast-in mounting rails[ ] \_\_\_\_\_ m BIRCOcanal NW 1000 channel without mounting rails[ ] Sealing with SF-Connectdelivery and installation according to manufacturer’s installation instructions.Manufacturer: BIRCO GmbHHerrenpfädel 142, D 76532 Baden-BadenPhone +497221 - 5003-0; Fax +497221 - 5003-1219; www.birco.de | **Unit price** | **Total price** |
| **BIRCOcanal NW 1000 – Covers**+ Width 1200 mm+ Height 165 mm+ 2 cast-in anchor sleeves RD 14 per cover for mechanical  installation[ ] \_\_\_\_\_ pce reinforced concrete cover with smooth surface  length 2000 mm, load class SLW 60delivery and installation according to manufacturer’s installation instructions.Manufacturer:BIRCO GmbH | **Unit price** | **Total price** |
| **BIRCOcanal NW 1000 – Cutting of channels including cover** [ ] \_\_\_\_\_ Channel section 90°[ ] \_\_\_\_\_ Mitre cut according to degree specificationManufacturer:BIRCO GmbH | **Unit price** | **Total price** |
| **BIRCOcanal NW 1000 – Drilled hole in channel base**[ ] \_\_\_\_\_ in horizontal / vertical direction, diameter DN 300Delivery.Manufacturer:BIRCO GmbH | **Unit price** | **Total price** |