|  |  |  |
| --- | --- | --- |
| **BIRCOcanal NW 300 – Supply channels with angles**  + External width 450 mm, internal width 300 mm  + External construction height 470 mm, internal height 350 mm  made of concrete C 40/50, CE compliance with EN 1433, up to load class F 900 as defined by EN 1433, with anchored 4 mm hot-dipped galvanized solid steel angles for combi-closure system (70 µm zinc coating), with safety sealing joint  [ ] \_\_\_\_\_ m BIRCOcanal NW 300 channel length 1000/2000 mm  with cast-in mounting rails  [ ] \_\_\_\_\_ m BIRCOcanal NW 300 channel length 1000/2000 mm  without mounting rails  [ ] Sealing with SF-Connect  including the necessary end caps, delivery and installation according to manufacturer’s installation instructions.  Manufacturer:  BIRCO GmbH Herrenpfädel 142, D 76532 Baden-Baden Phone +497221 - 5003-0; Fax +497221 - 5003-1219; www.birco.de | **Unit price** | **Total price** |
| **BIRCOcanal NW 300 – Gratings for supply channels with angles**  + Width 437 mm  + Height 45 mm  load class according to DIN EN 1433, with 8 point per metre M16/A2-bolt fastening or Easylock fastening  [ ] \_\_\_\_\_ pce bulb ductile iron cover(s) black immersion-  lacquered, length 500 mm, load class E 600  [ ] \_\_\_\_\_ pce bulb ductile iron cover(s) galvanized,   length 500 mm, load class E 600  delivery and installation according to manufacturer’s installation instructions.  Manufacturer:  BIRCO GmbH | **Unit price** | **Total price** |

|  |  |  |
| --- | --- | --- |
| **BIRCOcanal NW 300 – Supply channels without angles**  + External width 450 mm, internal width 300 mm  + External construction height 415 mm, internal height 340 mm  made of concrete C 40/50, CE compliance with EN 1433, up to load class E 600 as defined by EN 1433, with safety sealing joint  [ ] \_\_\_\_\_ m BIRCOcanal NW 300 channel length 1000/2000 mm   with cast-in mounting rails  [ ] \_\_\_\_\_ m BIRCOcanal NW 300 channel length 1000/2000 mm   without mounting rails  [ ] Sealing with SF-Connect  delivery and installation according to manufacturer’s installation instructions.  Manufacturer:  BIRCO GmbH Herrenpfädel 142, D 76532 Baden-Baden Phone +497221 - 5003-0; Fax +497221 - 5003-1219; www.birco.de | **Unit price** | **Total price** |
| **BIRCOcanal NW 300 – Covers for supply channels without angles**  + Width 450 mm  + Height 100 mm  + 2 cast-in anchor sleeves per cover for mechanical installation  [ ] \_\_\_\_\_ pce reinforced concrete cover with smooth surface  length 1000 mm, load class SLW 60  delivery and installation according to manufacturer’s installation instructions.  Manufacturer:  BIRCO GmbH | **Unit price** | **Total price** |
| **BIRCOcanal NW 300 – Cutting of channels including grating** and painting or galvanizing of cut angles and gratings.  [ ] \_\_\_\_\_ Channel section 90°  [ ] \_\_\_\_\_ Mitre cut according to degree specification  Manufacturer:  BIRCO GmbH | **Unit price** | **Total price** |
| **BIRCOcanal NW 300 – Drilled hole in channel base**  [ ] \_\_\_\_\_ in horizontal / vertical direction, diameter DN 300  Delivery.  Manufacturer:  BIRCO GmbH | **Unit price** | **Total price** |