|  |  |  |
| --- | --- | --- |
| **BIRCOcanal NW 500 – Supply channels with angles** with integrated two-sided anchoring system (AS) made of concrete  + External width at angle 650, at ground 690 mm  + Internal width 500 mm  + External construction height 550 mm, internal height 415 mm  made of concrete C 40/50, CE compliance with EN 1433, up to load class F 900 as defined by EN 1433, with anchored 4 mm hot-dipped galvanized solid steel angles for combi-closure system (70 µm zinc coating), with safety sealing joint  [ ] \_\_\_\_\_ m BIRCOcanal NW 500 AS channel length 1000 mm,  with cast-in mounting rails  [ ] \_\_\_\_\_ m BIRCOcanal NW 500 AS channel length 1000 mm,  without mounting rails  [ ] Sealing with SF-Connect  including the necessary end caps, delivery and installation according to manufacturer’s installation instructions.  Manufacturer:  BIRCO GmbH Herrenpfädel 142, D 76532 Baden-Baden Phone +497221 - 5003-0; Fax +497221 - 5003-1219; www.birco.de | **Unit price** | **Total price** |
| **BIRCOcanal NW 500 AS – Gratings for supply channels with angles**  + Width 633 mm  + Height 45 mm  load class according to DIN EN 1433, with 8 point per metre M16/A2-bolt fastening or Easylock fastening  [ ] \_\_\_\_\_ pce bulb ductile iron cover(s) black immersion-  lacquered, length 500 mm, load class E 600  delivery and installation according to manufacturer’s installation instructions.  Manufacturer: BIRCO GmbH | **Unit price** | **Total price** |

|  |  |  |
| --- | --- | --- |
| **BIRCOcanal NW 500 AS – Supply channels without angles** with integrated two-sided anchoring system (AS) made of concrete  + External width 650 mm, internal width 690 mm  + External construction height 500 mm, internal height 410 mm  made of concrete C 40/50, CE compliance with EN 1433, up to load class F 900 as defined by EN 1433, with safety sealing joint  [ ] \_\_\_\_\_ m BIRCOcanal NW 500 AS channel length 1000 mm   with cast-in mounting rails  [ ] \_\_\_\_\_ m BIRCOcanal NW 500 AS channel length 1000 mm   without mounting rails  [ ] Sealing with SF-Connect  delivery and installation according to manufacturer’s installation instructions.  Manufacturer:  BIRCO GmbH Herrenpfädel 142, D 76532 Baden-Baden Phone +497221 - 5003-0; Fax +497221 - 5003-1219; www.birco.de | **Unit price** | **Total price** |
| **BIRCOcanal NW 500 AS – Covers for supply channels without angles**  + Smoothed surface  [ ] \_\_\_\_\_ pce concrete cover length 5000 mm   until 1 m height above ground  [ ] \_\_\_\_\_ pce reinforced concrete cover length 1000 mm  load class SLW 60  delivery and installation according to manufacturer’s installation instructions.  Manufacturer: BIRCO GmbH | **Unit price** | **Total price** |
| **BIRCOcanal NW 500 AS – Drilled hole in channel base**  [ ] \_\_\_\_\_ in horizontal / vertical direction, diameter DN 300  Delivery.  Manufacturer: BIRCO GmbH | **Unit price** | **Total price** |