|  |  |  |
| --- | --- | --- |
| **BIRCOcanal NW 700 – Supply channels without angles**  + Lenght 2000 mm  + External width 900 mm, internal width 700 mm  + External construction height 500 mm, internal height 400 mm  + Cast-in anchor sleeves RD14 per cover for mechanical installation  made of reinforced grade concrete C 40/50, CE compliance with EN 1433, up to load class E 600 as defined by EN 1433, with safety sealing joint  [ ] \_\_\_\_\_ m BIRCOcanal NW 700 channel   with cast-in mounting rails  [ ] \_\_\_\_\_ m BIRCOcanal NW 700 channel without mounting rails  [ ] Sealing with SF-Connect  delivery and installation according to manufacturer’s installation instructions.  Manufacturer:  BIRCO GmbH Herrenpfädel 142, D 76532 Baden-Baden Phone +497221 - 5003-0; Fax +497221 - 5003-1219; www.birco.de | **Unit price** | **Total price** |
| **BIRCOcanal NW 700 – Covers for supply channels without angles**  + Width 900 mm  + Height 125 mm  + 2 cast-in anchor sleeves RD 14 per cover for mechanical installation  [ ] \_\_\_\_\_ pce reinforced concrete cover with smooth surface  length 2000 mm, load class SLW 60  delivery and installation according to manufacturer’s installation instructions.  Manufacturer: BIRCO GmbH | **Unit price** | **Total price** |
| **BIRCOcanal NW 700 – Cutting of channels including grating**  [ ] \_\_\_\_\_ Channel section 90°  [ ] \_\_\_\_\_ Mitre cut according to degree specification  Manufacturer: BIRCO GmbH | **Unit price** | **Total price** |
| **BIRCOcanal NW 700 – Drilled hole in channel base**  [ ] \_\_\_\_\_ in horizontal / vertical direction, diameter DN 300  Delivery.  Manufacturer: BIRCO GmbH | **Unit price** | **Total price** |