|  |  |  |
| --- | --- | --- |
| **BIRCOlight NW 150 AS – Drainage channel with 0.5 % inbuilt fall** with integrated two-sided anchoring system (AS) made of concrete+ Length 1000 mm+ Width at angle 210 mm, width at bottom 244 mm+ Construction height at groove/tongue 230 to 280 mmmade of concrete C 40/50 according to EN 1433, up to load class E 600 as defined by EN 1433, with anchored 4 mm hot-dipped galvanized solid steel angles and combi-closure toggle, with safety sealing joint[ ] \_\_\_\_\_ m BIRCOlight NW 150 AS channel No. 1 - 10[ ] Sealing with SF-Connectincluding the necessary end caps, delivery and installation according to manufacturer’s instructions.Manufacturer: BIRCO GmbHHerrenpfädel 142, D 76532 Baden-BadenPhone +497221 - 5003-0; Fax +497221 - 5003-1219; www.birco.de | **Unit price** | **Total price** |
| **BIRCOlight NW 150 AS – Drainage channel without inbuilt fall** with integrated two-sided anchoring system (AS) made of concrete+ Length 500 mm (heights 230 mm)/1000 mm+ Width at angle 210 mm, width at bottom 244 mm+ Construction height 230/255/280/305/325 mmmade of concrete C 40/50 according to EN 1433, up to load class E 600 as defined by EN 1433, with anchored 4 mm hot-dipped galvanized solid steel angles and combi-closure toggle, with safety sealing joint[ ] \_\_\_\_\_ m BIRCOlight NW 100 AS channel No. 0/0, 5/0, 10/0, 15/0, 20/0[ ] Sealing with SF-Connectincluding the necessary end caps, delivery and installation according to manufacturer’s instructions.Manufacturer: BIRCO GmbH | **Unit price** | **Total price** |
| **BIRCOlight NW 150 – End caps and end caps with outlet DN 150**+ Width 210 mmmade of galvanized steel[ ] \_\_\_\_\_ pce. of end cap(s) for channel no. 0/0 – 4 / 5/0 – 8 / 9 – 10 / 20/0[ ] \_\_\_\_\_ pce. of end cap(s) with outlet DN 150 No. 0/0 / 5/0 /  10/0 / 20/0delivery.Manufacturer: BIRCO GmbH | **Unit price** | **Total price** |

|  |  |  |
| --- | --- | --- |
| **BIRCOlight NW 150 AS –In-line outfall unit** for 1- or 2-sided channel connection with integrated two-sided anchoring system (AS) made of concrete+ Length at angle 500 mm, length at bottom 510 mm+ Width at angle 210 mm, width at bottom 260 mm,made of concrete C 40/50 according to EN 1433, PP silt bucket, integrated sockets for DN 100 pipe connection, with anchored 4 mm hot-dipped galvanized solid steel angles (70 µm zinc coating) and combi-closure toggle, with safety sealing joint[ ] \_\_\_\_\_ pce. In-line outfall unit, single piece, construction  height 710 mm, integrated sockets for DN 150 pipe  connection[ ] Sealing with SF-Connectincluding the necessary end caps, delivery and installation according to manufacturer’s instructions.Manufacturer:BIRCO GmbH | **Unit price** | **Total price** |
| **BIRCOlight NW 150 AS – Gratings**+ Width 200 mm+ Height 20 mmload class according to DIN EN 1433, with 2 point per metre M12/A2-bolt fastening or Easylock fastening[ ] \_\_\_\_\_ pce. ductile iron slotted gratings black immersion- lacquered, length 500 mm, load class C 250 / E 600[ ] \_\_\_\_\_ pce. ductile iron mesh gratings black immersion- lacquered, length 500 mm, load class C 250 / E 600[ ] \_\_\_\_\_ pce. mesh grating made of hot-dipped galvanized steel,  mesh width 30/15 mm, length 500 / 1000 mm, load  class C 250[ ] \_\_\_\_\_ pce. longitudinal bar gratings made of hot-dipped  galvanized steel, length 500 / 1000 mm, load class  C 250delivery and installation according to manufacturer’s instructions.Manufacturer:BIRCO GmbH | **Unit price** | **Total price** |
| **BIRCOlight NW 150 AS – Cutting of channels including grating** and painting or galvanizing of cut angles and gratings. For mesh gratings welding of end pieces and galvanizing.[ ] \_\_\_\_\_ Channel section 90°[ ] \_\_\_\_\_ Mitre cut according to degree specificationManufacturer:BIRCO GmbH | **Unit price** | **Total price** |

|  |  |  |
| --- | --- | --- |
| **BIRCOlight NW 150 AS – Hole drilling of channel**[ ] \_\_\_\_\_ in horizontal / vertical direction, diameter DN 150[ ] \_\_\_\_\_ pce. of silt bucket(s)delivery.Manufacturer:BIRCO GmbH | **Unit price** | **Total price** |