|  |  |  |
| --- | --- | --- |
| **BIRCOlight triloc NW 200 – Drainage channel with 0.5 % inbuilt fall** with integrated two-sided anchoring system (AS) made of concrete, with easy maintenance, clasp locking system+ Length 1000 mm+ Width at angle 262 mm, width at bottom 294 mm+ Construction height at groove/tongue 310 to 360 mmmade of concrete C 40/50 according to EN 1433, up to load class D 400 as defined by EN 1433, with anchored 4 mm hot-dipped galvanized solid steel angles, with safety sealing joint[ ] \_\_\_\_\_ m BIRCOlight triloc NW 200 **with BIRCOtriloc  fast locking system**, channel No. 1 – 10[ ] \_\_\_\_\_ m BIRCOlight triloc NW 200 **with M8 bolt  fastening**, channel No. 1 - 10[ ] Sealing with SF-Connectincluding the necessary end caps, delivery and installation according to manufacturer’s instructions.Manufacturer: BIRCO GmbHHerrenpfädel 142, D 76532 Baden-BadenPhone +497221 - 5003-0; Fax +497221 - 5003-1149; www.birco.de | **Unit price** | **Total price** |
| **BIRCOlight triloc NW 200 – Drainage channel without inbuilt fall** with integrated two-sided anchoring system (AS) made of concrete, with easy maintenance, clasp locking system+ Length 500 mm (heights 310 mm)/1000 mm+ Width at angle 262 mm, width at bottom 294 mm+ Construction height 310/330/360/410 mmmade of concrete C 40/50 according to EN 1433, up to load class D 400 as defined by EN 1433, with anchored 4 mm hot-dipped galvanized solid steel angles, with safety sealing joint[ ] \_\_\_\_\_ m BIRCOlight NW 200 AS triloc **with BIRCOtriloc  fast locking system**, channel No. 0/0, 5/0, 10/0,  20/0[ ] \_\_\_\_\_ m BIRCOlight NW 200 AS triloc **with M8 bolt  fastening**, channel No. 0/0, 5/0, 10/0, 20/0[ ] Sealing with SF-Connectincluding the necessary end caps, delivery and installation according to manufacturer’s instructions.Manufacturer: BIRCO GmbH | **Unit price** | **Total price** |

|  |  |  |
| --- | --- | --- |
| **BIRCOlight triloc NW 200 – End caps and end caps with outlet DN 200**+ Width 260 mmmade of galvaniszd steel[ ] \_\_\_\_\_ pce. of end cap(s) for channel no. 0/0 – 4 / 5/0 – 8 / 9 – 10 / 20/0[ ] \_\_\_\_\_ pce. of end cap(s) with outlet DN 200 No. 0/0 / 5/0 /  10/0 / 20/0delivery.Manufacturer: BIRCO GmbH | **Unit price** | **Total price** |
| **BIRCOlight NW 200 AS triloc –In-line outfall unit** for 1- or 2-sided channel connection with integrated two-sided anchoring system (AS) made of concrete, easy maintenance, clasp locking system+ Length at angle 500 mm, length at bottom 500 mm+ Width at angle 262 mm, width at bottom 304 mm,made of concrete C 40/50, up to load class D 400 as defined by EN 1433, PP silt bucket, with anchored 4 mm hot-dipped galvanized solid steel angles (70 µm zinc coating), with safety sealing joint[ ] \_\_\_\_\_ pce. In-line outfall unit **with BIRCOtriloc fast  locking system**, single piece, construction height  730 mm, integrated sockets for DN 200 pipe  connection[ ] \_\_\_\_\_ pce. In-line outfall unit **with M8 bolt fastening**,  single piece, construction height 730 mm, integrated  sockets for DN 200 pipe connection[ ] Sealing with SF-Connectincluding the necessary end caps, delivery and installation according to manufacturer’s instructions.Manufacturer:BIRCO GmbH | **Unit price** | **Total price** |
| **BIRCOlight NW 200 AS triloc – Grating**+ Length 500 mm+ Width 250 mm+ Height 20 mmup to load class D 400 as defined by EN 1433 [ ] \_\_\_\_\_ pce. ductile iron slotted gratings black immersion- lacquered, **with BIRCOtriloc fast locking system**[ ] \_\_\_\_\_ pce. ductile iron slotted gratings black immersion- lacquered, **with bolt fastening**delivery and installation according to manufacturer’s instructions.Manufacturer:BIRCO GmbH | **Unit price** | **Total price** |

|  |  |  |
| --- | --- | --- |
| **BIRCOlight NW 200 AS triloc – Cutting of channels including grating** and painting or galvanizing of cut angles and gratings. For mesh gratings welding of end pieces and galvanizing.[ ] \_\_\_\_\_ Channel section 90°[ ] \_\_\_\_\_ Mitre cut according to degree specificationManufacturer:BIRCO GmbH | **Unit price** | **Total price** |
| **BIRCOlight NW 200 AS triloc – Hole drilling of channel**[ ] \_\_\_\_\_ in horizontal / vertical direction, diameter DN 200  (vertical hole drilling until channel No. 10/0 max.  DN 150)[ ] \_\_\_\_\_ pce. of silt bucket(s)delivery.Manufacturer:BIRCO GmbH | **Unit price** | **Total price** |