|  |  |  |
| --- | --- | --- |
| **BIRCOlight triloc NW 200 – Drainage channel with  0.5 % inbuilt fall** with integrated two-sided anchoring system (AS) made of concrete, with easy maintenance, clasp locking system  + Length 1000 mm  + Width at angle 262 mm, width at bottom 294 mm  + Construction height at groove/tongue 310 to 360 mm  made of concrete C 40/50 according to EN 1433, up to load class D 400 as defined by EN 1433, with anchored 4 mm hot-dipped galvanized solid steel angles, with safety sealing joint  [ ] \_\_\_\_\_ m BIRCOlight triloc NW 200 **with BIRCOtriloc   fast locking system**, channel No. 1 – 10  [ ] \_\_\_\_\_ m BIRCOlight triloc NW 200 **with M8 bolt   fastening**, channel No. 1 - 10  [ ] Sealing with SF-Connect  including the necessary end caps, delivery and installation according to manufacturer’s instructions.  Manufacturer:  BIRCO GmbH Herrenpfädel 142, D 76532 Baden-Baden Phone +497221 - 5003-0; Fax +497221 - 5003-1149; www.birco.de | **Unit price** | **Total price** |
| **BIRCOlight triloc NW 200 – Drainage channel without inbuilt fall** with integrated two-sided anchoring system (AS) made of concrete, with easy maintenance, clasp locking system  + Length 500 mm (heights 310 mm)/1000 mm  + Width at angle 262 mm, width at bottom 294 mm  + Construction height 310/330/360/410 mm  made of concrete C 40/50 according to EN 1433, up to load class D 400 as defined by EN 1433, with anchored 4 mm hot-dipped galvanized solid steel angles, with safety sealing joint  [ ] \_\_\_\_\_ m BIRCOlight NW 200 AS triloc **with BIRCOtriloc   fast locking system**, channel No. 0/0, 5/0, 10/0,   20/0  [ ] \_\_\_\_\_ m BIRCOlight NW 200 AS triloc **with M8 bolt   fastening**, channel No. 0/0, 5/0, 10/0, 20/0  [ ] Sealing with SF-Connect  including the necessary end caps, delivery and installation according to manufacturer’s instructions.  Manufacturer:  BIRCO GmbH | **Unit price** | **Total price** |

|  |  |  |
| --- | --- | --- |
| **BIRCOlight triloc NW 200 – End caps and end caps with outlet DN 200**  + Width 260 mm  made of galvaniszd steel  [ ] \_\_\_\_\_ pce. of end cap(s) for channel no. 0/0 – 4 / 5/0 – 8 / 9 – 10 / 20/0  [ ] \_\_\_\_\_ pce. of end cap(s) with outlet DN 200 No. 0/0 / 5/0 /   10/0 / 20/0  delivery.  Manufacturer:  BIRCO GmbH | **Unit price** | **Total price** |
| **BIRCOlight NW 200 AS triloc –In-line outfall unit** for 1- or 2-sided channel connection with integrated two-sided anchoring system (AS) made of concrete, easy maintenance, clasp locking system  + Length at angle 500 mm, length at bottom 500 mm  + Width at angle 262 mm, width at bottom 304 mm,  made of concrete C 40/50, up to load class D 400 as defined by EN 1433, PP silt bucket, with anchored 4 mm hot-dipped galvanized solid steel angles (70 µm zinc coating), with safety sealing joint  [ ] \_\_\_\_\_ pce. In-line outfall unit **with BIRCOtriloc fast   locking system**, single piece, construction height   730 mm, integrated sockets for DN 200 pipe   connection  [ ] \_\_\_\_\_ pce. In-line outfall unit **with M8 bolt fastening**,   single piece, construction height 730 mm, integrated   sockets for DN 200 pipe connection  [ ] Sealing with SF-Connect  including the necessary end caps, delivery and installation according to manufacturer’s instructions.  Manufacturer: BIRCO GmbH | **Unit price** | **Total price** |
| **BIRCOlight NW 200 AS triloc – Grating**  + Length 500 mm  + Width 250 mm  + Height 20 mm  up to load class D 400 as defined by EN 1433  [ ] \_\_\_\_\_ pce. ductile iron slotted gratings black immersion-  lacquered, **with BIRCOtriloc fast locking system**  [ ] \_\_\_\_\_ pce. ductile iron slotted gratings black immersion-  lacquered, **with bolt fastening**  delivery and installation according to manufacturer’s instructions.  Manufacturer: BIRCO GmbH | **Unit price** | **Total price** |

|  |  |  |
| --- | --- | --- |
| **BIRCOlight NW 200 AS triloc – Cutting of channels including grating** and painting or galvanizing of cut angles and gratings. For mesh gratings welding of end pieces and galvanizing.  [ ] \_\_\_\_\_ Channel section 90°  [ ] \_\_\_\_\_ Mitre cut according to degree specification  Manufacturer: BIRCO GmbH | **Unit price** | **Total price** |
| **BIRCOlight NW 200 AS triloc – Hole drilling of channel**  [ ] \_\_\_\_\_ in horizontal / vertical direction, diameter DN 200   (vertical hole drilling until channel No. 10/0 max.   DN 150)  [ ] \_\_\_\_\_ pce. of silt bucket(s)  delivery.  Manufacturer: BIRCO GmbH | **Unit price** | **Total price** |