|  |  |  |
| --- | --- | --- |
| **BIRCOmassiv NW 200 – Drainage channel type I without inbuilt fall**  + Width at angle 500 mm, width at bottom 505 mm  + Construction height 415 mm  + With 8-point per metre anti-sliding safety studs of the grating  made of constructively reinforced concrete C 40/50, CE compliance with EN 1433, up to load class F 900 as defined by EN 1433, with anchored one-piece hot-dipped galvanized surface protection, with safety sealing joint  [ ] \_\_\_\_\_ m BIRCOmassiv NW 200 channel No. 0/0, with   galvanized surface protection,   length 1000 / 2000 mm  [ ] Sealing with SF-Connect  including the necessary end caps, delivery and installation according to manufacturer’s installation instructions.  Manufacturer:  BIRCO GmbH Herrenpfädel 142, D 76532 Baden-Baden Phone +497221 - 5003-0; Fax +497221 - 5003-1219; www.birco.de | **Unit price** | **Total price** |
| **BIRCOmassiv NW 200 – End caps and end caps with outlet DN 150**  + Width 500 mm  + for construction height 415 mm  made of galvanized steel  [ ] \_\_\_\_\_ pce. of end cap(s)  [ ] \_\_\_\_\_ pce. of end cap(s) with outlet DN 200  delivery.  Manufacturer:  BIRCO GmbH | **Unit price** | **Total price** |
| **BIRCOmassiv NW 200 – Ring nut M12**  + For installation of concrete channels  made of galvanized steel  [ ] \_\_\_\_\_ pce of ring nut(s)  delivery.  Manufacturer: BIRCO GmbH | **Unit price** | **Total price** |

|  |  |  |
| --- | --- | --- |
| **BIRCOmassiv NW 200 – In-line outfall unit** for 1- or 2-sided channel connection  + Length 500 mm  + Width at angle 500 mm, width at bottom 500mm  + With 4-point anti-sliding safety studs of the grating  made of constructively reinforced concrete C 40/50, CE compliance with EN 1433, up to load class F 900 as defined by EN 1433, with anchored one-piece hot-dipped galvanized surface protection, with safety sealing joint  [ ] \_\_\_\_\_ pce of in-line outfall unit(s), 1 piece, construction   height 980 mm, with galvanized surface protection,  integrated socket for DN 200 pipe connection, without   odour trap  [ ] Sealing with SF-Connect  including the necessary end caps, delivery and installation according to manufacturer’s installation instructions.  Manufacturer:  BIRCO GmbH | **Unit price** | **Total price** |
| **BIRCOmassiv NW 200 – Gratings**  + Width 287 mm  + Height 30 mm  load class according to DIN EN 1433, 8 point per metre M12/A2 self-locking nuts  [ ] \_\_\_\_\_ pce ductile iron slotted gratings black immersion-  lacquered, length 500 mm, load class E 600 / F 900  [ ] \_\_\_\_\_ pce ductile iron honeycomb gratings black immersion-  lacquered, length 500 mm, load class E 600 / F 900  delivery and installation according to manufacturer’s installation instructions  Manufacturer: BIRCO GmbH | **Unit price** | **Total price** |
| **BIRCOmassiv NW 200 – Cutting of channels including grating** and painting or galvanizing of cut angles and gratings.  [ ] \_\_\_\_\_ Channel section 90°  [ ] \_\_\_\_\_ Mitre cut according to degree specification  Manufacturer:  BIRCO GmbH | **Unit price** | **Total price** |
| **BIRCOmassiv NW 200 – Hole drilling of channel**  [ ] \_\_\_\_\_ in horizontal / vertical direction, diameter DN 200  [ ] \_\_\_\_\_ pce of silt bucket(s)  Delivery.  Manufacturer:  BIRCO GmbH | **Unit price** | **Total price** |