|  |  |  |
| --- | --- | --- |
| **BIRCOsir NW 100 – Drainage channel with 1 % inbuilt fall**  + Length 1000 mm  + Width at angle 200 mm, width at bottom 205 mm  + Construction height at groove/tongue 180 to 330 mm  made of concrete C 40/50 according to EN 1433, up to load class D 400 Type I / F 900 Type M as defined by EN 1433, with anchored 4 mm hot-dipped galvanized solid steel angles for combi-closure system (70 µm zinc coating), with safety sealing joint  [ ] \_\_\_\_\_ m BIRCOsir NW 100 channel No. 1 - 15  [ ] Sealing with SF-Connect  including necessary end caps, delivery and installation according to manufacturer’s installation instructions.  Manufacturer:  BIRCO GmbH Herrenpfädel 142, D 76532 Baden-Baden Phone +497221 - 5003-0; Fax +497221 - 5003-1149; www.birco.de | **Unit price** | **Total price** |
| **BIRCOsir NW 100 – Drainage channel without inbuilt fall**  + Length 500 mm (just height 180 mm)/1000 mm  + Width at angle 200 mm, width at bottom 205 mm  + Construction height 180/230/280/330 mm  made of concrete C 40/50 according to EN 1433, up to load class F 900 as defined by EN 1433, with anchored 4 mm hot-dipped galvanized solid steel angles for combi-closure system (70 µm zinc coating), with safety sealing joint  [ ] \_\_\_\_\_ m BIRCOsir NW 100 channel No. 0/0, 5/0, 10/0, 15/0  [ ] Sealing with SF-Connect  including necessary end caps, delivery and installation according to manufacturer’s installation instructions.  Manufacturer:  BIRCO GmbH | **Unit price** | **Total price** |
| **BIRCOsir NW 100 – Shallow channel without inbuilt fall**  + Length 1000 mm  + Width at angle 200 mm, width at bottom 205 mm  + Construction height 80/100/150/200 mm  made of concrete C 40/50 according to EN 1433, up to load class F 900 as defined by EN 1433, with anchored 4 mm hot-dipped galvanized solid steel angles for combi-closure system (70 µm zinc coating), with safety sealing joint  [ ] \_\_\_\_\_ m BIRCOsir NW 100 shallow channel construction   height 80/100/150/200  [ ] Sealing with SF-Connect  including necessary end caps, delivery and installation according to manufacturer’s installation instructions.  Manufacturer: BIRCO GmbH | **Unit price** | **Total price** |
| **BIRCOsir NW 100 – End caps and end caps with outlet DN 100**  + Width 200 mm  made of galvanized steel  [ ] \_\_\_\_\_ pce. of end cap(s) for channel no. 0/0–2 / 3–4 / 5–6 /  7–8 / 9–10/0 / 11–12 / 13–14 / 15–15/0  [ ] \_\_\_\_\_ pce. of end cap(s) for shallow channel,   construction height 80-100 / 150 / 200 mm  [ ] \_\_\_\_\_ pce. of end cap(s) with outlet DN 100 for channel   no. 0/0 / 5/0 / 10/0 / 15/0  delivery.  Manufacturer:  BIRCO GmbH | **Unit price** | **Total price** |
| **BIRCOsir NW 100 – In-line outfall unit** for 1- or 2-sided channel connection  + Length 500 mm  + Width at angle 200 mm, width at bottom 230 mm  + PP silt bucket  made of concrete C 40/50 according to EN 1433, up to load class F 900 as defined by EN 1433, with anchored 4 mm hot-dipped galvanized solid steel angles for combi-closure system (70 µm zinc coating), with safety sealing joint  [ ] \_\_\_\_\_ pce in-line outfall unit, 1 piece, construction height 490 mm, integrated socket for DN 100 pipe connection including socket plug, PP odour trap for channel No. 0/0 - 10  [ ] \_\_\_\_\_ pce in-line outfall unit, 1 piece, construction height 695 mm, integrated socket for DN 150 (without odour trap) pipe connection, socket plug for channel No. 0/0 to 15  [ ] Sealing with SF-Connect  including necessary end caps, delivery and installation according to manufacturer’s installation instructions.  Manufacturer:  BIRCO GmbH | **Unit price** | **Total price** |

|  |  |  |
| --- | --- | --- |
| **BIRCOsir NW 100 – Gratings**  + Width 187 mm  + Height 30 mm  load class according to DIN EN 1433, with 8-point per meter M12/A2-bolt fastening or Easylock fastening, mesh grating  4 point fastening per grating  [ ] \_\_\_\_\_ pce ductile iron slotted grating black immersion-  lacquered, length 500 mm, load class C 250 / D 400 /   E 600 / F 900  [ ] \_\_\_\_\_ pce. ductile iron slotted grating black immersion-  lacquered, narrow slot, length 500 mm, load class   E 600  [ ] \_\_\_\_\_ pce ductile iron mesh grating black immersion-  lacquered, length 500 mm, load class E 600  [ ] \_\_\_\_\_ pce mesh grating galvanized steel,   length 500 / 1000 mm,   mesh width 30/12 mm, load class C 250  mesh width 20/30 mm, load class E 600 delivery and installation according to manufacturer’s installation instructions.  Manufacturer:  BIRCO GmbH | **Unit price** | **Total price** |
| **BIRCOsir NW 100 – Cutting of channels including grating** and painting or galvanizing of cut angles and gratings. For mesh gratings welding of end pieces and galvanizing.  [ ] \_\_\_\_\_ 90° cut  [ ] \_\_\_\_\_ Mitre cut according to degree specification  Manufacturer:  BIRCO GmbH | **Unit price** | **Total price** |
| **BIRCOsir NW 100 – Hole drilling of channel**  [ ] \_\_\_\_\_ in horizontal / vertical direction, diameter DN 100  [ ] \_\_\_\_\_ pce of silt bucket(s)  [ ] \_\_\_\_\_ pce of silt bucket(s) for shallow channels  Delivery.  Manufacturer:  BIRCO GmbH | **Unit price** | **Total price** |