|  |  |  |
| --- | --- | --- |
| **BIRCOsir NW 200 AS – Drainage channel with 0.5 % inbuilt fall** with integrated two-sided anchoring system (AS) made of concrete+ Length 1000 mm+ Width at angle 300 mm, width at bottom 332 mm+ Construction height at groove/tongue 310 to 360 mmmade of concrete C 40/50 according to EN 1433, up to load class D 400 Type I / F 900 Type M as defined by EN 1433, with anchored 4 mm hot-dipped galvanized solid steel angles for combi-closure system (70 µm zinc coating), with safety sealing joint[ ] \_\_\_\_\_ m BIRCOsir NW 200 AS channel No. 1 – 10[ ] Sealing with SF-Connectincluding necessary end caps, delivery and installation according to manufacturer’s installation instructions.Manufacturer: BIRCO GmbHHerrenpfädel 142, D 76532 Baden-BadenPhone +497221 - 5003-0; Fax +497221 - 5003-1149; www.birco.de | **Unit price** | **Total price** |
| **BIRCOsir NW 200 AS – – Drainage channel without inbuilt fall** with integrated two-sided anchoring system (AS) made of concrete+ Length 500 mm (just height 310 mm)/1000 mm+ Width at angle 300 mm, width at bottom 332 mm+ Construction height 310/335/360/410 mmmade of concrete C 40/50 according to EN 1433, up to load class D 400 Type I / F 900 Type M as defined by EN 1433, with anchored 4 mm hot-dipped galvanized solid steel angles for combi-closure system (70 µm zinc coating), with safety sealing joint[ ] \_\_\_\_\_ m BIRCOsir NW 200 AS channel No. 0/0, 5/0, 10/0,  20/0[ ] Sealing with SF-Connectincluding necessary end caps, delivery and installation according to manufacturer’s installation instructions.Manufacturer:BIRCO GmbH | **Unit price** | **Total price** |

|  |  |  |
| --- | --- | --- |
| **BIRCOsir NW 200 AS – Shallow channel without inbuilt fall** with integrated two-sided anchoring system (AS) made of concrete+ Length 1000 mm+ Width at angle 300 mm, width at bottom 334 mm+ Construction height 200 / 250 mmmade of concrete C 40/50 according to EN 1433, up to load class E 600 as defined by EN 1433, with anchored 4 mm hot-dipped galvanized solid steel angles for combi-closure system (70 µm zinc coating), with safety sealing joint[ ] \_\_\_\_\_ m BIRCOsir NW 200 AS shallow channel construction  height 200/250[ ] Sealing with SF-Connectincluding necessary end caps, delivery and installation according to manufacturer’s installation instructions.Manufacturer:BIRCO GmbH | **Unit price** | **Total price** |
| **BIRCOsir NW 200 AS – End caps and end caps with outlet DN 200**+ Width 330 mmmade of galvanized steel[ ] \_\_\_\_\_ pce. of end cap(s) for channel no. 0/0–5/0 / 6–10/0 / 20/0[ ] \_\_\_\_\_ pce. of end cap(s) for shallow channel,  construction height 200 / 250 mm[ ] \_\_\_\_\_ pce. of end cap(s) with outlet DN 200 for channel  no. 0/0 / 5/0 / 10/0 / 20/0delivery.Manufacturer: BIRCO GmbH | **Unit price** | **Total price** |

|  |  |  |
| --- | --- | --- |
| **BIRCOsir NW 200 AS – – In-line outfall unit** for 1- or 2-sided channel connection,with integrated two-sided anchoring system (AS) made of concrete+ Length at angle 500 mm, Length at bottom 510 mm+ Width at angle 300 mm, width at bottom 345 mm,+ Galvanized silt bucket+ Without odour trapmade of concrete C 40/50 according to EN 1433, up to load class F 900 as defined by EN 1433, with anchored 4 mm hot-dipped galvanized solid steel angles for combi-closure system (70 µm zinc coating), with safety sealing joint[ ] \_\_\_\_\_ pce in-line outfall unit, 1 piece, construction height  740 mm, integrated socket for DN 200 pipe  connection[ ] Sealing with SF-Connectincluding necessary end caps, delivery and installation according to manufacturer’s installation instructions.Manufacturer:BIRCO GmbH | **Unit price** | **Total price** |
| **BIRCOsir NW 200 AS – Gratings**+ Width 287 mm+ Height 30 mmload class according to DIN EN 1433, with 8-point per meter M12/A2-bolt fastening or Easylock fastening, mesh grating 4 point fastening per grating[ ] \_\_\_\_\_ pce ductile iron slotted grating black immersion- lacquered, length 500 mm, load class D 400 / E 600 /  F 900[ ] \_\_\_\_\_ pce ductile iron mesh grating black immersion- lacquered, length 500 mm, load class C 250 / E 600[ ] \_\_\_\_\_ pce ductile iron honeycomb gratings black immersion- lacquered, length 500 mm, load class E 600 / F 900[ ] \_\_\_\_\_ pce mesh grating galvanized steel,  length 500 / 1000 mm, mesh width 30/30, load class C 250delivery and installation according to manufacturer’s installation instructions.Manufacturer:BIRCO GmbH | **Unit price** | **Total price** |
| **BIRCOsir NW 200 AS – Cutting of channels including grating** and painting or galvanizing of cut angles and gratings. For mesh gratings welding of end pieces and galvanizing. [ ] \_\_\_\_\_ 90° cut[ ] \_\_\_\_\_ Mitre cut according to degree specificationManufacturer:BIRCO GmbH | **Unit price** | **Total price** |

|  |  |  |
| --- | --- | --- |
| **BIRCOsir NW 200 AS – Hole drilling of channel**[ ] \_\_\_\_\_ in horizontal / vertical direction, diameter DN 200[ ] \_\_\_\_\_ pce of silt bucket(s)[ ] \_\_\_\_\_ pce of silt bucket(s) for shallow channelsDelivery.Manufacturer:BIRCO GmbH | **Unit price** | **Total price** |