|  |  |  |
| --- | --- | --- |
| **BIRCOsir NW 300 AS – Drainage channel with 0.5% inbuilt fall** with integrated two-sided anchoring system (AS) made of concrete+ Length 1000 mm, 2000 mm+ Width at angle 430 mm, width at bottom 470 mm+ Construction height 410 mm to 550 mmmade of concrete C 40/50 according to EN 1433, up to load class D 400 Type I / F 900 Type M as defined by EN 1433, with anchored 4 mm hot-dipped galvanized solid steel angles for combi-closure system (70 µm zinc coating), with safety sealing joint[ ] \_\_\_\_\_ m BIRCOsir NW 300 AS channel construction  No. 1 - 28, length 1000 / 2000 mm[ ] Sealing with SF-Connectincluding necessary end caps, delivery and installation according to manufacturer’s installation instructions.Manufacturer: BIRCO GmbHHerrenpfädel 142, D 76532 Baden-BadenPhone +497221 - 5003-0; Fax +497221 - 5003-1149; www.birco.de | **Unit price** | **Total price** |
| **BIRCOsir NW 300 AS – Drainage channel without inbuilt fall** with integrated two-sided anchoring system (AS) made of concrete+ Length 1000 mm, 2000 mm+ Width at angle 430 mm, width at bottom 470 mm+ Construction height 1: 410 mm/ Construction height 2: 550 mmmade of concrete C 40/50 according to EN 1433, up to load class D 400 Type I / F 900 Type M as defined by EN 1433, with anchored 4 mm hot-dipped galvanized solid steel angles for combi-closure system (70 µm zinc coating), with safety sealing joint[ ] \_\_\_\_\_ m BIRCOsir NW 300 AS channel construction  height 1 / 2, length 1000 / 2000 mm[ ] Sealing with SF-Connectincluding necessary end caps, delivery and installation according to manufacturer’s installation instructions.Manufacturer: BIRCO GmbHHerrenpfädel 142, D 76532 Baden-BadenPhone +497221 - 5003-0; Fax +497221 - 5003-1149; www.birco.de | **Unit price** | **Total price** |

|  |  |  |
| --- | --- | --- |
| **BIRCOsir NW 300 AS – Shallow channel without inbuilt fall** with integrated two-sided anchoring system (AS) made of concrete+ Length 1000 mm+ Width at angle 430 mm, width at bottom 470 mm+ Construction height 300 mmmade of concrete C 40/50 according to EN 1433, up to load class E 600 as defined by EN 1433, with anchored 4 mm hot-dipped galvanized solid steel angles for combi-closure system (70 µm zinc coating), with safety sealing joint[ ] \_\_\_\_\_ m BIRCOsir NW 300 AS shallow channel[ ] Sealing with SF-Connectincluding necessary end caps, delivery and installation according to manufacturer’s installation instructions.Manufacturer: BIRCO GmbH | **Unit price** | **Total price** |
| **BIRCOsir NW 300 AS – End caps and end caps with outlet DN 200**+ Width 430 mmmade of galvanized steel[ ] \_\_\_\_\_ pce. of end cap(s) for channel construction height 1 / 2[ ] \_\_\_\_\_ pce. of end cap(s) for shallow channel[ ] \_\_\_\_\_ pce. of end cap(s) with outlet DN 200 for channel  construction height 1 / 2delivery.Manufacturer:BIRCO GmbH | **Unit price** | **Total price** |
| **BIRCOsir NW 300 AS – In-line outfall unit** for 1- or 2-sided channel connection,with integrated two-sided anchoring system (AS) made of concrete+ Length 500 m+ Width at angle 430 mm, width at bottom 460mm+ Galvanized silt bucket+ Integrated socket for DN 300 pipe connection+ Without odour trapmade of concrete C 40/50 according to EN 1433, up to load class F 900 as defined by EN 1433, with anchored 4 mm hot-dipped galvanized solid steel angles for combi-closure system (70 µm zinc coating), with safety sealing joint[ ] \_\_\_\_\_ pce in-line outfall unit, 1 piece, construction height  980 mm[ ] Sealing with SF-Connectincluding necessary end caps, delivery and installation according to manufacturer’s installation instructions.Manufacturer: BIRCO GmbH | **Unit price** | **Total price** |

|  |  |  |
| --- | --- | --- |
| **BIRCOsir NW 300 AS – Gratings**+ Width 417 mm+ Height 35 mmload class according to DIN EN 1433, with 8-point per meter M12/A2-bolt fastening or Easylock fastening, mesh grating 4 point fastening per grating[ ] \_\_\_\_\_ pce ductile iron twofold slotted grating black  immersion- lacquered, length 500 mm,  load class D 400 / E 600 / F 900[ ] \_\_\_\_\_ pce ductile iron mesh grating black immersion- lacquered, length 500 mm, load class C 250 / E 600[ ] \_\_\_\_\_ pce bulb ducitile iron cover, black immersion- lacquered, length 500 mm, load class E 600delivery and installation according to manufacturer’s installation instructions.Manufacturer: BIRCO GmbH | **Unit price** | **Total price** |
| **BIRCOsir NW 300 AS – Cutting of channels including grating** and painting or galvanizing of cut angles and gratings. For mesh gratings welding of end pieces and galvanizing. [ ] \_\_\_\_\_ 90° cut[ ] \_\_\_\_\_ Mitre cut according to degree specificationManufacturer:BIRCO GmbH | **Unit price** | **Total price** |
| **BIRCOsir NW 300 AS – Hole drilling of channel**[ ] \_\_\_\_\_ in horizontal / vertical direction, diameter DN 300[ ] \_\_\_\_\_ pce of silt bucket(s)[ ] \_\_\_\_\_ pce of silt bucket(s) for shallow channelsDelivery.BIRCO GmbH | **Unit price** | **Total price** |