|  |  |  |
| --- | --- | --- |
| **BIRCOsir NW 400 – Drainage channel without inbuilt fall**+ Length 1000 mm / 2000 mm+ Width at angle 550 mm, width at bottom 560 mm+ Construction height 480 mmmade of concrete C 40/50 according to EN 1433, up to load class D 400 Type I / F 900 Type M as defined by EN 1433, with anchored 4 mm hot-dipped galvanized solid steel angles for combi-closure system (70 µm zinc coating), with safety sealing joint[ ] \_\_\_\_\_ m BIRCOsir NW 400 channel[ ] Sealing with SF-Connectincluding necessary end caps, delivery and installation according to manufacturer’s installation instructions.Manufacturer: BIRCO GmbHHerrenpfädel 142, D 76532 Baden-BadenPhone +497221 - 5003-0; Fax +497221 - 5003-1149; www.birco.de | **Unit price** | **Total price** |
| **BIRCOsir NW 400 – End caps and end caps with outlet DN 300**+ Width 550 mm+ for construction height 480 mmmade of galvanized steel[ ] \_\_\_\_\_ pce. of end cap(s) for channel no. 0/0 [ ] \_\_\_\_\_ pce. of end cap(s) with outlet DN 300 for channel  no. 0/0delivery.Manufacturer:BIRCO GmbH | **Unit price** | **Total price** |
| **BIRCOsir NW 400 – In-line outfall unit** for 1- or 2-sided channel connection + Length 500 mm+ Width at angle 550 mm, width at bottom 550mm+ Galvanized silt bucket+ Integrated socket for DN 300 pipe connection+ Without odour trapmade of concrete C 40/50 according to EN 1433, up to load class F 900 as defined by EN 1433, with anchored 4 mm hot-dipped galvanized solid steel angles for combi-closure system (70 µm zinc coating), with safety sealing joint[ ] \_\_\_\_\_ pce in-line outfall unit, 1 piece, construction height  980 mm[ ] Sealing with SF-Connectincluding necessary end caps, delivery and installation according to manufacturer’s installation instructions.Manufacturer:BIRCO GmbH | **Unit price** | **Total price** |

|  |  |  |
| --- | --- | --- |
| **BIRCOsir NW 400 – Gratings**+ Width 537 mm+ Height 45 mmload class according to DIN EN 1433, with 8-point per metre M16/A2-bolt fastening or Easylock fastening [ ] \_\_\_\_\_ pce ductile iron twofold slotted grating black  immersion-lacquered, length 500 mm,  load class D 400 / E 600 / F 900[ ] \_\_\_\_\_ pce ductile iron mesh grating black immersion- lacquered, length 500 mm, load class E 600delivery and installation according to manufacturer’s installation instructions.Manufacturer:BIRCO GmbH | **Unit price** | **Total price** |
| **BIRCOsir NW 400 – Cutting of channels including grating** and painting or galvanizing of cut angles and gratings.[ ] \_\_\_\_\_ 90° cut[ ] \_\_\_\_\_ Mitre cut according to degree specificationManufacturer:BIRCO GmbH | **Unit price** | **Total price** |
| **BIRCOsir NW 400 – Hole drilling of channel**[ ] \_\_\_\_\_ in horizontal / vertical direction, diameter DN 300[ ] \_\_\_\_\_ pce of silt bucket(s)Delivery.Manufacturer:BIRCO GmbH | **Unit price** | **Total price** |