|  |  |  |
| --- | --- | --- |
| **BIRCOsir NW 500 AS – Channel without inbuilt fall** with integrated two-sided anchoring system (AS) made of concrete  + Length 1000 mm  + Width at angle 650 mm, width at bottom 690 mm  + Construction height 550 mm  made of concrete C 40/50 according to EN 1433, up to load class D 400 Type I / F 900 Type M as defined by EN 1433, with anchored 4 mm hot-dipped galvanized solid steel angles for combi-closure system (70 µm zinc coating), with safety sealing joint  [ ] \_\_\_\_\_ m BIRCOsir NW 500 AS channel  [ ] Sealing with SF-Connect  including the necessary end caps, delivery and installation according to the installation instructions of the producer.  Producer:  BIRCO GmbH Herrenpfädel 142, D 76532 Baden-Baden Phone +497221 - 5003-0; Fax +497221 - 5003-1149; www.birco.de | **Unit price** | **Total price** |
| **BIRCOsir NW 500 AS - End caps and end caps with outlet  DN 300**  + Width 650 mm  + For construction height 550 mm  made of galvanized steel  [ ] \_\_\_\_\_ pce. of end cap(s) for channel no. 0/0  [ ] \_\_\_\_\_ pce. of end cap(s) with outlet DN 300 for channel   no. 0/0  delivery.  Producer:  BIRCO GmbH | **Unit price** | **Total price** |
| **BIRCOsir NW 500 AS – Grating**  + Width 633 mm  + Height 45 mm  load class according to DIN EN 1433, with 8 point per meter M16/A2-bolt fastening or Easylock fastening  [ ] \_\_\_\_\_ pce ductile iron threefold slotted gratings, black  immersion- lacquered, length 500 mm, load class   D 400 / E 600 / F 900  delivery and installation according to the installation instructions of the producer  Producer:  BIRCO GmbH | **Unit price** | **Total price** |

|  |  |  |
| --- | --- | --- |
| **BIRCOsir NW 500 AS – Cutting of channels including grating** and painting or galvanizing of cutted angles and gratings.  [ ] \_\_\_\_\_ Channel section 90°  [ ] \_\_\_\_\_ Mitre cut according to degree specification  Producer:  BIRCO GmbH | **Unit price** | **Total price** |
| **BIRCOsir NW 500 AS – Hole drilling of channel**  [ ] \_\_\_\_\_ in horizontal / vertical direction, diameter DN 300  delivery.  Producer:  BIRCO GmbH | **Unit price** | **Total price** |